|  |  |  |
| --- | --- | --- |
| LLD Version | Updates | Author |
| 1. 0 | Initial Version for Phase1a | Rhoda |
| 1. 1 | Added Response parameter mapping | Rhoda |
| 1.2 | Updated HLR template mapping | Rhoda |
| 1.3 | Phase 1a command mapping updates | Rhoda |
| 1.4 | Rework: based on final Phase1a command mappng | Rhoda |
| 1.5 | Freeze version for Phase1a | Rhoda |
| 1.6 | Based on Phase 1b command mapping | Triveni |
| 1.7 | Catalog Mapping for 1b | Rhoda |
| 1.8 | Catalog Mapping for 1b: Added CHGIMSI commands for missed NEI's | Triveni |
| 1.9 | Catalog Mapping for 1b: Added FMS, ISM, ATS, ENUM and phase 1b HLR transactions | Triveni |
| 2.0 | Added FLP commands - based on freeze version Trident Wireless Optima RFS Command Mapping\_202005281707.xlsx | Rhoda |
| 2.1 | Added HLR templates for FLP | Rhoda |
| 2.2 | Catalog Mapping for Wireline: IPTV, SATTV and ND | Rhoda |
| 2.3 | Added entries for Smart Intra MNP | Reybal |
| 2.4 | Update CWS command in Intra MNP | Reybal |
| 2.5 | Update EDB command in Intra MNP | Reybal |
| 2.6 | Merge Catalog Wireline Mapping Added PLDT Home Wifi | Rhoda |
| 2.7 | Added CR 41 sheet based on Trident Commmand mapping revision 41.00 Impacts HLR template for LTE, DATA and DATAROAMING | Rhoda |
| 2.8 | Added ISM getNumberDetail for VOIP ND and NDLIFT (Catalog Wireline sheet) | Rhoda |
| 2.9 | Updated OneOCS Command for MPVOICE ADD and REMOVE in Intra MNP | Reybal |
| 3.0 | Simple Wireless Enterprise project updates: Added SFDC Enterprise sheet | Rhoda |
| 3.1 | Simple Wireless Enterprise project updates: Updated SFDC Enterprise sheet and Added SFDC HLR Template sheet based on Trident Wireless Optima RFS Command Mapping\_202011121209 | Rhoda |
| 3.2 | Simple Wireless Enterprise project updates: Updated SFDC Enterprise sheet and SFDC HLR Template sheet based on Trident Wireless Optima RFS Command Mapping\_202011151109 | Rhoda |
| 3.3 | Simple Wireless Enterprise project updates: Added special handling on DATA\_PROFILING - ADD AAA transaction | Rhoda |
| 3.4 | Simple Wireless Enterprise project updates: Updated HLR template for ROAMING\_ADD and ROAMING\_RESUME (IDC and CEBU) based on Trident Wireless Optima RFS Command Mapping\_202011261104.xlsx | Rhoda |
| 3.5 | Simple Wireless Enterprise project updates: Added CLIPOVERRIDE templates | Rhoda |
| 3.6 | Added PLP Fixed Wireless sheet based on Trident Wireless Optima RFS Command Mapping\_202011271717.xlsx | Rhoda |
| 3.7 | Updated PLP Fixed Wireless sheet based on Trident Wireless Optima RFS Command Mapping\_202012151103.xlsx - instead of updating existing MVOICE, introduced new RFS - MVOICE\_PLP | Rhoda |
| 3.8 | Updated Create/ADD HLR command for MPVOICE in Intra MNP | Reybal |
| 3.9 | 5G requirements - refer to 5G HLR changes and 5G catalog changes sheets EIRAVAS CR - pls refer to SFDC Enterprise sheet | Rhoda |
| 4.0 | Updated Create/ADD HLR command for MPVOICE in Intra MNP | Reybal |
| 4.1 | CALLHOLD CR refer to NE - ONENDS HLR (1b) sheet entry for CALLHOLD\_REMOVE | Rhoda |
| 4.2 | DP9 Rollback refer to Catalog Mapping (1a) sheet enty for MVOICE\_ADD DP9 | Rhoda |
| 4.3 | Additional task if error (0005/9999) is encountered in OTA in Intra MNP. | Reybal |
| 4.4 | Change Plan sheet | Rhoda |
| 4.5 | Added Prepaid ChangeIMSI and Prepaid ChangeIMSI HLR sheets | Rhoda |
| 4.6 | BARINCOMING/BAROUTGOING RESUME/SUSPEND CR - refer to BARRING sheet | Rhoda |
| 4.7 | Remove ONEOCS from MVOICE\_CHGIMSI for OPTIMA only, refer to MVOICE\_CHGIMSI sheet | Rhoda |
| 4.8 | Paywall Redirection and Paywall Redirection UNDO | Rhoda |
| 4.9 | Redirection CR based on command mapping T-USPS RFS Command Mapping\_202103240906.xlsx v. 74.0 Minor update on Paywall Redirection sheet - updated LTE RFS HLR condition | Rhoda |
| 5.0 | Paywall Redirection Catalog Mapping updates | Rhoda |
| 5.1 | Paywall Redirection Catalog Mapping updates - interchange DATA\_ADD and DATA\_REMOVE | Rhoda |
| 5.2 | Proposed HLR changes based on: T-USPS RFS Command Mapping\_202104191839.xlsx refer to Gate2 HLR templates | Rhoda |
| 5.3 | CWS changes on appending prefix 9 based on: T-USPS RFS Command Mapping\_202105041631.xlsx | Rhoda |
| 5.4 | Treatment and Redirection | Rhoda |
| 5.5 | BAROUTGOING RESUME | Rhoda |
| 5.6 | Based on version 86 of T-USPS RFS Command Mapping\_202105271828.xlsx | Rhoda |
| 5.7 | Modify DATA\_ADD | Rhoda |
| 5.8 | CRI changes sheet: MVOICE\_ADD (Create) MVOICE\_CHGNUMBER (Modify) | Rhoda |
| 5.9 | BAROUTGOING sheet: Based on version 88 of T-USPS RFS Command Mapping\_202107062004.xlsx | Rhoda |
| 6.0 | Added INM for PLP Fixed wireless - PLP INM sheet | Rhoda |
| 6.1 | BARINCOMING CR | Rhoda |
| 6.2 | DSL\_TOPUP | Rhoda |
| 6.3 | Project Bright: Phase1 MVOICE - ADD, CHGIMSI, CHGNUMBER | Rhoda |
| 6.4 | Project Bright: Phase2 USSD | Heena |
| 6.5 | Project Bright:  CRI Fixes Phase1 Rollback Transactions | Rhoda |
| 6.6 | Project Bright:  Phase2 - MVOICE, VOLTE | Heena |
| 6.7 | Project Bright:  Phase1 - OCS command updates for Create/Modify MVOICE ADD | Rhoda |
| 6.8 | Project Bright - Change in USSD NEI parameters - As per changes by Amdocs in USSD NEI FSD | Heena |
| 6.9 | IOT Connectivity Management: IOT Catalog IOT Templates | Rhoda |
| 7.0 | Intra MNP: 1. Change the status from 2 to 1 in OCS command (CreateSubscriber) for MPVOICE ADD 2. Add rollback command in OCS command for MVOICE ADD 3. Add rollback command in OCS command for MPVOICE ADD | Rhoda |
| 7.1 | Wireless Optiima 1. Update UPCC parameter mapping for TRANSACTIONID for all applicable use cases | Rhoda |
| 7.2 | Free Apple Music Promo: 1. Phase 1 and 2, MVOICE - SUBSCRIBE, CHGNUMBER, CHGOWNERSHIP, SUSPEND | Kamhoong |
| 7.3 | Infinity CR: New WIFI RFS introduced for Infinity CR. | Kamhoong |
| 7.4 | Added sheet for DTS Direct catalog call requests. | Reybal |
| 7.5 | Merge the InterMNP related sheet and added InterMNP for Non-DSA | Kamhoong |
| 7.6 | Updated InterMNP for Non-DSA sheet on ISM PORT\_IN\_ACT changes Added BILLCAP CR Updated AGW and CDP isRoam value from 0 to 1 for ADD | Kamhoong |
| 7.7 | Added ATS VOLTE CR Catalog, additional ATS command for RFS\_VOLTE (RFS\_Command\_Mapping version 108) | Kamhoong |
| 7.8 | Added new tabs IMS CORE InterMNP, IMS CORE Templates and IMS CORE Catalog (RFS\_Command\_Mapping version 110) | Kamhoong |
| 7.9 | Added new tabs Peloton FMO InterMNP and Peloton FMO Catalog (RFS\_Command\_Mapping version 112)  06042022 update: added MVOICE INTER REMOVE | Kamhoong |
| 8.0 | Added new tabs CWS-WS Application Decommissioning  (RFS\_Command\_Mapping version 119) | Kamhoong |
| 8.1 | Added new tab SIMReg-Ph3-NewPrepaidSimProfile (RFS\_Command\_Mapping version 123/125) | Kamhoong |
| 8.2 | Added new tab CallForkingForWearablesOtherDev (RFS\_Command\_Mapping version 118) | Kamhoong |
| 8.3 | Added new tab SimRegPostpaidDr1 Catalog, SimRegPostpaidDrop1(InterMNP), SimRegPostpDr1(InterMNPNon-DSA) Impacted use case: • ADD-\_MVOICE (New Connect) • ADD-\_MVOICE\_INTRA (Intra MNP - Change brand to Postpaid) • ADD-\_MPVOICE\_INTRA (Intra MNP - Change brand to Prepaid) • PREACT-\_MVOICE\_INTER (Inter MNP Postpaid Port in using DSA SIM) • ADD-\_MVOICE\_INTER (Inter MNP Postpaid Port in using Non-DSA SIM) (RFS\_Command\_Mapping version 127) | Kamhoong |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Catalog item** | **Transaction** | **NETWORK ELEMENT** | **Technical Service** | **Parameters** | **ACTIONCODE/CONDITION** | **ROLLBACK/REVERSAL** | **Expected command** | **Sequence command** |
| RFS\_MVOICE | SUBSCRIBE | HLR | TS\_HLR\_ONENDS\_V9\_DUMMY | NE\_TYPE=HLR | skiptask |  | USE\_TEMPLATE=MVOICE\_SUBSCRIBE |  |
| RFS\_INTERNET | SUBSCRIBE | VUPCC |  | SERVICE NAME, SUBSCRIPTION END DATE (yyyymmddhhmmss) | POST exec IF error, Generate parameters: NEID\_1,RFS\_1,ERROR\_CODE\_1,ERROR\_MSG\_1 via Map command   POST exec IF Error FAIL SO | UNSUBSCRIBE | <ns2:subscribeService  xmlns:ns2="rm:soap">  <inPara>  <subscriber>  <attribute>  <key>usrIdentifier</key>  <value><MSISDN></value>  </attribute>  </subscriber>  <subscribedService>  <attribute>  <key>srvName</key>  <value><SERVICE NAME></value>  </attribute>  <attribute>  <key>TransACTIONCODEID</key>  <value>201912061345033076058</value>  </attribute>  <attribute>  <key>srvSubscribeDate</key>  <value><CURRENT DATE/TIME></value>  </attribute>  <attribute>  <key>srvStartDateTime</key>  <value><CURRENT DATE/TIME></value>  </attribute>  <attribute>  <key>srvEndDateTime</key>  <value><SUBSCRIPTION END DATE></value>  </attribute>  <attribute>  <key>srvCreateSubscriber</key>  <value>1</value>  </attribute>  <attribute>  <key>usrMSISDN</key>  <value><MSISDN></value>  </attribute>  <attribute>  <key>usrPaidType</key>  <value>1</value>  </attribute>  </subscribedService>  </inPara> </ns2:subscribeService> |  |
| RFS\_OCS\_OFFER | SUBSCRIBE | OCS |  |  | POST exec IF error, Generate parameters: NEID\_1,RFS\_1,ERROR\_CODE\_1,ERROR\_MSG\_1 via Map command   POST exec IF Error FAIL SO | refer to NE - ONEOCS sheet | refer to NE - ONEOCS sheet |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **<RFS>\_<ACTION>** | | | | **SPML** | | | | **Parameters** |
| CALID\_ADD | | | | <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <clip>true</clip>  </valueObject>  </modification> | | | |  |
| CALID\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification name="hlr/clip" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| CALID\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification name="hlr/clip" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| CALID\_RESUME | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <clip>true</clip>  </valueObject>  </modification> </request> | | | | IMSI |
| CFB\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFB">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFB">  <basicServiceGroup>BS20-dataAsync</basicServiceGroup>  <status>4</status>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFB">  <basicServiceGroup>BS30-dataSync</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | | | |  |
| CFB\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/cfb" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| CFB\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification name="hlr/cfb" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| CFB\_RESUME | | | |  | | | |  |
| CFNRC\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFNrc">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFNrc">  <basicServiceGroup>BS20-dataAsync</basicServiceGroup>  <status>4</status>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFNrc">  <basicServiceGroup>BS30-dataSync</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | | | |  |
| CFNRC\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/cfnrc" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| CFNRC\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/cfnrc" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| CFNRC\_RESUME | | | |  | | | |  |
| CFNRY\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFNry">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFNry">  <basicServiceGroup>BS20-dataAsync</basicServiceGroup>  <status>4</status>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFNry">  <basicServiceGroup>BS30-dataSync</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | | | |  |
| CFNRY\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/cfnry" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| CFNRY\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/cfnry" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| CFNRY\_RESUME | | | |  | | | |  |
| CFU\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFU">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFU">  <basicServiceGroup>BS20-dataAsync</basicServiceGroup>  <status>4</status>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:CFU">  <basicServiceGroup>BS30-dataSync</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | | | |  |
| CFU\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/cfu" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| CFU\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/cfu" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| CFU\_RESUME | | | |  | | | |  |
| DATA\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <gprs>  <msisdn><MSISDN></msisdn>  </gprs>  <generalChargingCharacteristics>  <chargingCharacteristicsProfile><CHARGING PROFILE></chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior><CHARGING BEHAVIOR></chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs><ODBGPRS></odbgprs>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:PDPContext">  <id><PDP ID></id>  <type>2</type>  <qosProfile><QOS></qosProfile>  <apn><APN NAME></apn>  <apnArea>HPLMN</apnArea>  </valueObject>  </modification> </request> | | | | ODBGPRS, PDP ID, QOS, APN NAME, CHARGING PROFILE, CHARGING BEHAVIOR |
| DATA\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/gprs" operation="remove" scope="uniqueTypeMapping"/>  <modification name="hlr/generalChargingCharacteristics[@chargingCharacteristics='normal']" operation="remove"></modification>  <modification name="hlr/pdpContext[@apn='<APN NAME>']" operation="remove"></modification> </request> | | | | ODBGPRS, PDP ID, QOS, APN NAME, CHARGING PROFILE, CHARGING BEHAVIOR |
| DATA\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs><ODBGPRS></odbgprs>  </valueObject>  </modification> </request> | | | | ODBGPRS, PDP ID, QOS, APN NAME, CHARGING PROFILE, CHARGING BEHAVIOR |
| DATA\_RESUME | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs><ODBGPRS></odbgprs>  </valueObject>  </modification> </request> | | | | ODBGPRS, PDP ID, QOS, APN NAME, CHARGING PROFILE, CHARGING BEHAVIOR |
| DATA\_CHGNUMBER | | | | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><MSISDN></oldId>  <newId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><NEW MSISDN></newId> </request> | | | | MSISDN NEW\_MSISDN |
| DATA\_CHGIMSI | | | | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><IMSI></oldId>  <newId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><NEW IMSI></newId> </request> | | | | IMSI NEW\_IMSI |
| GPRS\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:PDPContext">  <id><PDP ID></id>  <type>2</type>  <qosProfile><QOS></qosProfile>  <apn><APN NAME></apn>  <apnArea>HPLMN</apnArea>  </valueObject>  </modification> </request> | | | | IMSI PDP\_ID QOS APN\_NAME |
| GPRS\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/pdpContext[@apn='<APN NAME>']" operation="remove"></modification> </request> | | | | IMSI APN\_NAME |
| IDD\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odboc>0</odboc>  </valueObject>  </modification> </request> | | | | IMSI |
| IDD\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odboc>2</odboc>  </valueObject>  </modification> </request> | | | | IMSI |
| IDD\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odboc>2</odboc>  </valueObject>  </modification> </request> | | | | IMSI |
| IDD\_RESUME | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odboc>0</odboc>  </valueObject>  </modification> </request> | | | | IMSI |
| INTERNET\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs><ODBGPRS></odbgprs>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <obGprs>0</obGprs>  </valueObject>  </modification>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps><ODBPOACCESSEPS></odbPOAccessEps>  </valueObject>  </modification> </request> | | | | IMSI ODBGPRS ODBPOACCESSEPS |
| INTERNET\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>2</odbgprs>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <obGprs>0</obGprs>  </valueObject>  </modification>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps>ALLPOS</odbPOAccessEps>  </valueObject>  </modification> </request> | | | | IMSI |
| INTERNET\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>1</odbgprs>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <obGprs>0</obGprs>  </valueObject>  </modification>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps>VPLMNAP</odbPOAccessEps>  </valueObject>  </modification> </request> | | | | IMSI |
| INTERNET\_RESUME | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs><ODBGPRS></odbgprs>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <obGprs>0</obGprs>  </valueObject>  </modification>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps><ODBPOACCESSEPS></odbPOAccessEps>  </valueObject>  </modification> </request> | | | | IMSI ODBGPRS ODBPOACCESSEPS |
| LTE\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId><DEF PDP ID></defaultPdnContextId>  <maxBandwidthUp><DEF MAX UPLOAD></maxBandwidthUp>  <maxBandwidthDown><DEF MAX DOWNLOAD></maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn><MSISDN></msisdn>  <odbPOAccessEps><LTE ACCESS></odbPOAccessEps>  </eps>  <epsPdnContext>  <apn><APN NAME></apn>  <contextId><PDP ID></contextId>  <type>both</type>  <maxBandwidthUp><MAX UPLOAD></maxBandwidthUp>  <maxBandwidthDown><MAX DOWNLOAD></maxBandwidthDown>  <qos><QOS></qos>  </epsPdnContext>  </valueObject>  </modification> </request> | | | | DEFAULT PDP ID, MAX UPLOAD, MAX DOWNLOAD, APN NAME xx, PDP ID xx, QOS xx |
| LTE\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/eps" operation="remove"></modification>  <modification name="hlr/epsPdnContext" operation="remove"></modification> </request> | | | | IMSI |
| LTE\_RESUME | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps><LTE ACCESS></odbPOAccessEps>  </valueObject>  </modification> </request> | | | | IMSI |
| LTE\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps><LTE ACCESS></odbPOAccessEps>  </valueObject>  </modification> </request> | | | | IMSI |
| MVOICE\_ADD\_IDC | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <imsiActive>true</imsiActive>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <sr>9</sr>  <odboc>2</odboc>  <odbic>0</odbic>  <odboprc>0</odboprc>  <odbssm>0</odbssm>  <odbsci>0</odbsci>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <bs20genr>  <msisdn><MSISDN></msisdn>  </bs20genr>  <bs30genr>  <msisdn><MSISDN></msisdn>  </bs30genr>  <cuss>  <status>2</status>  </cuss>  <basicSelfLocation>  <status>2</status>  </basicSelfLocation>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <routingCategory><ROUTCAT></routingCategory>  <supportNewRadioSecondaryRAT>true</supportNewRadioSecondaryRAT>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | | | |  |
| MVOICE\_ADD\_CEB | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <imsiActive>true</imsiActive>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <sr>9</sr>  <odboc>2</odboc>  <odbic>0</odbic>  <odboprc>0</odboprc>  <odbssm>0</odbssm>  <odbsci>0</odbsci>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <bs20genr>  <msisdn><MSISDN></msisdn>  </bs20genr>  <bs30genr>  <msisdn><MSISDN></msisdn>  </bs30genr>  <cuss>  <status>2</status>  </cuss>  <basicSelfLocation>  <status>2</status>  </basicSelfLocation>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <routingCategory><ROUTCAT></routingCategory>  <supportNewRadioSecondaryRAT>true</supportNewRadioSecondaryRAT>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | | | |  |
| MVOICE\_SUBSCRIBE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | | | |  |
| MVOICE\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/> </request> | | | | IMSI |
| MVOICE\_UNSUBSCRIBE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>5</status>  </valueObject>  </modification> </request> <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>5</status>  </valueObject>  </modification> </request> | | | |  |
| MVOICE\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>5</status>  </valueObject>  </modification> </request> <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>5</status>  </valueObject>  </modification> </request> | | | |  |
| MVOICE\_RESUME | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | | | |  |
| MVOICE\_CHGNUMBER | | | | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><MSISDN></oldId>  <newId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><NEW MSISDN></newId> </request> | | | | MSISDN NEW\_MSISDN |
| MVOICE\_CHGIMSI | | | | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><IMSI></oldId>  <newId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><NEW IMSI></newId> </request> | | | | IMSI NEW\_IMSI |
| MVOICE\_CHGNUMBER\_RB | | | | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><NEW MSISDN></oldId>  <newId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><MSISDN></newId> </request> | | | | MSISDN NEW\_MSISDN |
| MVOICE\_CHGIMSI\_RB | | | | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><NEW IMSI></oldId>  <newId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><IMSI></newId> </request> | | | | IMSI NEW\_IMSI |
| ROAMING\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <sr>9</sr>  </valueObject>  </modification>  <modification name="hlr/rr" operation="remove" scope="uniqueTypeMapping"/>  <modification name="hlr/roamSubscription" operation="remove" scope="uniqueTypeMapping"/>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | | | | ODBGPRS, PDP ID, QOS, APN NAME, CHARGING PROFILE, CHARGING BEHAVIOR |
| ROAMING\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <rr>RPI\_all</rr>  <sr>1</sr>  </valueObject>  </modification>  <modification name="hlr/roamSubscription" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:ROAMSUBSCRIPTION">  <roamSubscriptionInfo>PTPD\_DFT10</roamSubscriptionInfo>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSIR1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCIR1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | | | |  |
| ROAMING\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <rr>RPI\_all</rr>  <sr>1</sr>  </valueObject>  </modification>  <modification name="hlr/roamSubscription" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:ROAMSUBSCRIPTION">  <roamSubscriptionInfo>PTPD\_DFT10</roamSubscriptionInfo>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSIR1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCIR1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | | | |  |
| ROAMING\_RESUME | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <sr>9</sr>  </valueObject>  </modification>  <modification name="hlr/rr" operation="remove" scope="uniqueTypeMapping"/>  <modification name="hlr/roamSubscription" operation="remove" scope="uniqueTypeMapping"/>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | | | |  |
| SMSO\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ts22>  <msisdn><MSISDN></msisdn>  </ts22>  </valueObject>  </modification> </request> | | | | IMSI |
| SMSO\_CHGIMSI | | | | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><IMSI></oldId>  <newId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><NEW IMSI></newId> </request> | | | | IMSI |
| SMSO\_CHGNUMBER | | | | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><MSISDN></oldId>  <newId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><NEW MSISDN></newId> </request> | | | |  |
| SMSO\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/ts22" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| SMSO\_RESUME | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS20-shortMessage</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | | | | MSISDN NEW\_MSISDN |
| SMSO\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS20-shortMessage</basicServiceGroup>  <status>5</status>  </valueObject>  </modification> </request> | | | | IMSI NEW\_IMSI |
| SMST\_ADD | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ts21>  <msisdn><MSISDN></msisdn>  </ts21>  </valueObject>  </modification> </request> | | | | MSISDN |
| SMST\_REMOVE | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/ts21" operation="remove" scope="uniqueTypeMapping"/> </request> | | | | IMSI |
| SMST\_SUSPEND | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS20-shortMessage</basicServiceGroup>  <status>5</status>  </valueObject>  </modification> </request> | | | | IMSI |
| SMST\_RESUME | | | | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS20-shortMessage</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | | | | IMSI |
| SMST\_CHGNUMBER | | | | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><MSISDN></oldId>  <newId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><NEW MSISDN></newId> </request> | | | | MSISDN NEW\_MSISDN |
| SMST\_CHGIMSI | | | | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><IMSI></oldId>  <newId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><NEW IMSI></newId> </request> | | | | IMSI NEW\_IMSI |
| HLR\_GEN\_BATCHREQUEST\_CREATE | | | | <spml:batchRequest  xmlns:spml="urn:siemens:names:prov:gw:SPML:2:0"  xmlns:subscriber="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" execution="synchronous" processing="sequential" onError="exit\_rollback" xsi:schemaLocation="urn:siemens:names:prov:gw:SUBSCRIBER:3:0 subscriber-3.0.xsd">  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  [${template1\_tmpl}]  [${template2\_tmpl}]  [${template3\_tmpl}]  ...  [${template12\_tmpl}] </request> </spml:batchRequest> | | | | template<priority>\_tmpl template1\_tmpl template2\_tmpl .. template12\_tmpl  Ex:  template1\_tmpl=MVOICE\_REMOVE.template |
| HLR\_GEN\_BATCHREQUEST\_CREATE | | | | soapenv:Body.spml:batchResponse.response.result=RESULT soapenv:Body.spml:batchResponse.response.requestID=REQUEST\_ID soapenv:Body.spml:batchResponse.response.errorCode=ERROR\_CODE soapenv:Body.spml:batchResponse.response.errorMessage=ERROR\_MESSAGE | | | |  |
| HLR\_GEN\_BATCHREQUEST\_MODIFY | | | | <spml:batchRequest  xmlns:spml="urn:siemens:names:prov:gw:SPML:2:0"  xmlns:subscriber="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" execution="synchronous" processing="sequential" onError="exit\_rollback" xsi:schemaLocation="urn:siemens:names:prov:gw:SUBSCRIBER:3:0 subscriber-3.0.xsd">  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  [${template1\_tmpl}]  [${template2\_tmpl}]  [${template3\_tmpl}]  ...  [${template12\_tmpl}] </request> </spml:batchRequest> | | | | template<priority>\_tmpl template1\_tmpl template2\_tmpl .. template12\_tmpl  Ex:  template1\_tmpl=MVOICE\_REMOVE.template |
| HLR\_GEN\_BATCHREQUEST\_MODIFY | | | | soapenv:Body.spml:batchResponse.response.result=RESULT soapenv:Body.spml:batchResponse.response.requestID=REQUEST\_ID soapenv:Body.spml:batchResponse.response.errorCode=ERROR\_CODE soapenv:Body.spml:batchResponse.response.errorMessage=ERROR\_MESSAGE | | | |  |
| HLR\_GEN\_BATCHREQUEST\_DELETE | | | | <spml:batchRequest  xmlns:spml="urn:siemens:names:prov:gw:SPML:2:0"  xmlns:subscriber="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" execution="synchronous" processing="sequential" onError="exit\_rollback" xsi:schemaLocation="urn:siemens:names:prov:gw:SUBSCRIBER:3:0 subscriber-3.0.xsd">  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  [${template1\_tmpl}]  [${template2\_tmpl}]  [${template3\_tmpl}]  ...  [${template12\_tmpl}] </request> </spml:batchRequest> | | | | template<priority>\_tmpl template1\_tmpl template2\_tmpl .. template12\_tmpl  Ex:  template1\_tmpl=MVOICE\_REMOVE.template |
| HLR\_GEN\_BATCHREQUEST\_DELETE | | | | soapenv:Body.spml:batchResponse.response.result=RESULT soapenv:Body.spml:batchResponse.response.requestID=REQUEST\_ID soapenv:Body.spml:batchResponse.response.errorCode=ERROR\_CODE soapenv:Body.spml:batchResponse.response.errorMessage=ERROR\_MESSAGE | | | |  |
| HLR\_GEN\_BATCHREQUEST\_RB | | | | <spml:batchRequest  xmlns:spml="urn:siemens:names:prov:gw:SPML:2:0"  xmlns:subscriber="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" execution="synchronous" processing="sequential" onError="exit\_rollback" xsi:schemaLocation="urn:siemens:names:prov:gw:SUBSCRIBER:3:0 subscriber-3.0.xsd">  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  [${rb\_template1\_tmpl}]  [${rb\_template2\_tmpl}]  [${rb\_template3\_tmpl}]  ...  [${rb\_template12\_tmpl}] </request> </spml:batchRequest> | | | | template<priority>\_tmpl rb\_template1\_tmpl rb\_template2\_tmpl .. rb\_template12\_tmpl  Ex:  rb\_template1\_tmpl=MVOICE\_REMOVE\_RB.template |
| HLR\_GEN\_BATCHREQUEST\_RB | | | | soapenv:Body.spml:batchResponse.response.result=RESULT soapenv:Body.spml:batchResponse.response.requestID=REQUEST\_ID soapenv:Body.spml:batchResponse.response.errorCode=ERROR\_CODE soapenv:Body.spml:batchResponse.response.errorMessage=ERROR\_MESSAGE | | | |  |
|  | | | |  | | | |  |
|  | | | |  | | | |  |
|  | | | |  | | | |  |
|  | | | |  | | | |  |
|  | | | |  | | | |  |
|  | | | |  | | | |  |
|  | | | |  | | | |  |
| **RFS** | **ACTION** | **NE** | **IDC command** | | **CEB Command** | **Sequence** | **Rollback Command** | | |
| OCS\_OFFER | ADD | ONEOCS | <ns8:CreateCustomerRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T17:36:25.7791265492813100799192926</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <CreateCustomerRequest>  <ns8:RegisterCustKey>***<ACCOUNT NUMBER>***/ns8:RegisterCustKey>  <ns8:Customer>  <ns8:CustKey>***<ACCOUNT NUMBER>***</ns8:CustKey>  <ns8:CustInfo>  <ns7:CustClass>1</ns7:CustClass>  <ns7:CustCode>***<ACCOUNT NUMBER>***</ns7:CustCode>  <ns7:CustBasicInfo>  <ns7:CustProperty>  <ns7:Code>C\_MSISDN\_FOR\_ROUTE</ns7:Code>  <ns7:Value>***<MSISDN>***</ns7:Value>  </ns7:CustProperty>  </ns7:CustBasicInfo>  </ns8:CustInfo>  </ns8:Customer>  <ns8:DFTAccount>  <ns8:PayRelationKey>***<ACCOUNT NUMBER>***</ns8:PayRelationKey>  <ns8:AcctKey>***<ACCOUNT NUMBER>***</ns8:AcctKey>  <ns8:AcctInfo>  <ns7:AcctCode>***<ACCOUNT NUMBER>***</ns7:AcctCode>  <ns7:BillCycleType>***<BILL CUTOFF DAY>***</ns7:BillCycleType>  <ns7:AcctType>1</ns7:AcctType>  <ns7:PaymentType>1</ns7:PaymentType>  <ns7:AcctClass>1</ns7:AcctClass>  <ns7:CurrencyID>1117</ns7:CurrencyID>  <ns7:InitBalance>0</ns7:InitBalance>  <ns7:AcctPayMethod>1</ns7:AcctPayMethod>  </ns8:AcctInfo>  </ns8:DFTAccount>  </CreateCustomerRequest> </ns8:CreateCustomerRequestMsg> | | same as IDC | 1 | <ns8:SubDeactivationRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T13:45:53.5742817311689992092934</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <SubDeactivationRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>3</ns8:OpType>  </SubDeactivationRequest> </ns8:SubDeactivationRequestMsg> | | |
| OCS\_OFFER | ADD | ONEOCS | <ChangeSubOfferingRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:SupplementaryOffering>  <ns8:AddOffering>  <ns7:OfferingKey>  <ns7:OfferingID><OCS OFFER ID></ns7:OfferingID>  </ns7:OfferingKey>  <ns8:EffectiveTime>  <ns7:Mode>I</ns7:Mode>  </ns8:EffectiveTime>  <ns8:ActivationTime/>  </ns8:AddOffering>  </ns8:SupplementaryOffering> </ChangeSubOfferingRequest> | | same as IDC | 2 | <ChangeSubOfferingRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:SupplementaryOffering>  <ns8:DelOffering>  <ns8:OfferingKey>  <ns7:OfferingID><OCS OFFER ID></ns7:OfferingID>  </ns8:OfferingKey>  </ns8:DelOffering>  </ns8:SupplementaryOffering>  <ns8:HandlingChargeFlag>1</ns8:HandlingChargeFlag> </ChangeSubOfferingRequest> | | |
| OCS\_OFFER | SUBSCRIBE | ONEOCS | <ns8:ChangeSubOfferingRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T17:40:31.42018801256739285001680</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeSubOfferingRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:SupplementaryOffering>  <ns8:AddOffering>  <ns7:OfferingKey>  <ns7:OfferingID>***<OCS OFFER ID>***</ns7:OfferingID>  </ns7:OfferingKey>  <ns8:EffectiveTime>  <ns7:Mode>I</ns7:Mode>  </ns8:EffectiveTime>  <ns8:ActivationTime/>  </ns8:AddOffering>  </ns8:SupplementaryOffering>  </ChangeSubOfferingRequest> </ns8:ChangeSubOfferingRequestMsg> | | same as IDC |  | <ns8:ChangeSubOfferingRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T17:43:21.79110112793919199915680</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeSubOfferingRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:SupplementaryOffering>  <ns8:DelOffering>  <ns8:OfferingKey>  <ns7:OfferingID>***<OCS OFFER ID>***</ns7:OfferingID>  </ns8:OfferingKey>  </ns8:DelOffering>  </ns8:SupplementaryOffering>  <ns8:HandlingChargeFlag>1</ns8:HandlingChargeFlag>  </ChangeSubOfferingRequest> </ns8:ChangeSubOfferingRequestMsg> | | |
| OCS\_OFFER | RESUME | ONEOCS | <ns8:ChangeSubStatusRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T13:54:25.8392980224929399712059</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeSubStatusRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>30</ns8:OpType>  </ChangeSubStatusRequest> </ns8:ChangeSubStatusRequestMsg> | | same as IDC |  | <ns8:ChangeSubStatusRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T10:15:30.90617998093069209089975</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeSubStatusRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>32</ns8:OpType>  </ChangeSubStatusRequest> </ns8:ChangeSubStatusRequestMsg> | | |
| OCS\_OFFER | SUSPEND | ONEOCS | <ns8:ChangeSubStatusRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T10:15:30.90617998093069209089975</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeSubStatusRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>32</ns8:OpType>  </ChangeSubStatusRequest> </ns8:ChangeSubStatusRequestMsg> | | same as IDC |  | <ns8:ChangeSubStatusRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T13:54:25.8392980224929399712059</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeSubStatusRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>30</ns8:OpType>  </ChangeSubStatusRequest> </ns8:ChangeSubStatusRequestMsg> | | |
| OCS\_OFFER | UNSUBSCRIBE |  | <ns8:SubDeactivationRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T13:45:53.5742817311689992092934</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <SubDeactivationRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>3</ns8:OpType>  </SubDeactivationRequest> </ns8:SubDeactivationRequestMsg> | | same as IDC |  |  | | |
| OCS\_OFFER | REMOVE | ONEOCS | <ns8:ChangeSubOfferingRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T17:43:21.79110112793919199915680</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeSubOfferingRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:SupplementaryOffering>  <ns8:DelOffering>  <ns8:OfferingKey>  <ns7:OfferingID>***<OCS OFFER ID>***</ns7:OfferingID>  </ns8:OfferingKey>  </ns8:DelOffering>  </ns8:SupplementaryOffering>  <ns8:HandlingChargeFlag>1</ns8:HandlingChargeFlag>  </ChangeSubOfferingRequest> </ns8:ChangeSubOfferingRequestMsg> | | same as IDC |  | <ns8:ChangeSubOfferingRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T17:40:31.42018801256739285001680</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeSubOfferingRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:SupplementaryOffering>  <ns8:AddOffering>  <ns7:OfferingKey>  <ns7:OfferingID>***<OCS OFFER ID>***</ns7:OfferingID>  </ns7:OfferingKey>  <ns8:EffectiveTime>  <ns7:Mode>I</ns7:Mode>  </ns8:EffectiveTime>  <ns8:ActivationTime/>  </ns8:AddOffering>  </ns8:SupplementaryOffering>  </ChangeSubOfferingRequest> </ns8:ChangeSubOfferingRequestMsg> | | |
| OCS\_OFFER | CHGNUMBER | ONEOCS | <ns8:ChangeSubIdentityRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T17:33:46.2572972118909189012914</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeSubIdentityRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:ModifySubIdentity>  <ns8:OldSubIdentity>***<MSISDN>***</ns8:OldSubIdentity>  <ns8:OldSubIdentityType>1</ns8:OldSubIdentityType>  <ns8:NewSubIdentity>***<NEW MSISDN>***</ns8:NewSubIdentity>  </ns8:ModifySubIdentity>  </ChangeSubIdentityRequest> </ns8:ChangeSubIdentityRequestMsg> | | same as IDC |  | <ns8:ChangeSubIdentityRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T17:33:46.2572972118909189012914</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeSubIdentityRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity>***<NEW MSISDN>***</ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:ModifySubIdentity>  <ns8:OldSubIdentity>***<NEW MSISDN>***</ns8:OldSubIdentity>  <ns8:OldSubIdentityType>1</ns8:OldSubIdentityType>  <ns8:NewSubIdentity>***<MSISDN>***</ns8:NewSubIdentity>  </ns8:ModifySubIdentity>  </ChangeSubIdentityRequest> </ns8:ChangeSubIdentityRequestMsg> | | |
| OCS\_OFFER | CHGIMSI | ONEOCS | <ChangeSubIdentityRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:ModifySubIdentity>  <ns8:OldSubIdentity><IMSI></ns8:OldSubIdentity>  <ns8:OldSubIdentityType>2</ns8:OldSubIdentityType>  <ns8:NewSubIdentity><NEW IMSI></ns8:NewSubIdentity>  </ns8:ModifySubIdentity> </ChangeSubIdentityRequest> | |  |  | <ChangeSubIdentityRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:ModifySubIdentity>  <ns8:OldSubIdentity><NEW IMSI></ns8:OldSubIdentity>  <ns8:OldSubIdentityType>2</ns8:OldSubIdentityType>  <ns8:NewSubIdentity><IMSI></ns8:NewSubIdentity>  </ns8:ModifySubIdentity> </ChangeSubIdentityRequest> | | |
| OCS\_OFFER | CHGBILLCYCLE | ONEOCS | <ns8:ChangeAcctBillCycleRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T17:09:41.202741369871100791480019</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeAcctBillCycleRequest>  <ns8:Account>  <ns8:RootAccount>  <ns7:AccountKey>***<ACCOUNT NUMBER>***</ns7:AccountKey>  </ns8:RootAccount>  </ns8:Account>  <ns8:NewBillCycleType>***<NEW BILL CUTOFF DAY>***</ns8:NewBillCycleType>  <ns8:EffectiveTime>  <ns7:Mode>N</ns7:Mode>  </ns8:EffectiveTime>  </ChangeAcctBillCycleRequest> </ns8:ChangeAcctBillCycleRequestMsg> | | same as IDC |  | <ns8:ChangeAcctBillCycleRequestMsg  xmlns:ns2="http://cbs.huawei.com/ar/wsservice/arcommon"  xmlns:ns4="http://www.huawei.com/bme/cbsinterface/arservices"  xmlns:ns3="http://www.huawei.com/bme/cbsinterface/cbscommon"  xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon"  xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices"  xmlns:ns7="http://www.huawei.com/bme/cbsinterface/bccommon"  xmlns:ns8="http://www.huawei.com/bme/cbsinterface/bcservices">  <RequestHeader>  <ns3:Version>1</ns3:Version>  <ns3:MessageSeq>2019-12-06T17:09:41.202741369871100791480019</ns3:MessageSeq>  <ns3:OwnershipInfo>  <ns3:BEID>102</ns3:BEID>  </ns3:OwnershipInfo>  <ns3:AccessSecurity>  <ns3:LoginSystemCode>uspsIT</ns3:LoginSystemCode>  <ns3:Password>S8Lq2miBr4q6TJW9bMRmR/4jk2MWnz/9FriXWC6Eemw=</ns3:Password>  </ns3:AccessSecurity>  <ns3:OperatorInfo>  <ns3:OperatorID>102</ns3:OperatorID>  </ns3:OperatorInfo>  <ns3:TimeFormat>  <ns3:TimeType>1</ns3:TimeType>  </ns3:TimeFormat>  </RequestHeader>  <ChangeAcctBillCycleRequest>  <ns8:Account>  <ns8:RootAccount>  <ns7:AccountKey>***<ACCOUNT NUMBER>***</ns7:AccountKey>  </ns8:RootAccount>  </ns8:Account>  <ns8:NewBillCycleType>***<OLD BILL CUTOFF DAY>***</ns8:NewBillCycleType>  <ns8:EffectiveTime>  <ns7:Mode>N</ns7:Mode>  </ns8:EffectiveTime>  </ChangeAcctBillCycleRequest> </ns8:ChangeAcctBillCycleRequestMsg> | | |
| OCS\_OFFER | CHGOWNERSHIP | ONEOCS |  | |  |  |  | | |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Catalog item** | **TransACTIONCODE** | **NETWORK ELEMENT** | **Technical Service** | **Parameters** | **Parameters/Attributes Internal to USPS** | **ACTIONCODE/CONDITION** | **Rollback/Reversal** | **Expected command** | **Sequence command** |
| RFS\_MVOICE | ADD\_NC | SSP | TS\_SSP\_SEG\_V1\_preactNWCON | SSPTYPE, IMSI |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | TXNCODE=GSM\_NWCON<tab>FICS1=***<MSISDN>***<tab>FICS2=***<IMSI>***<tab>FICS3=***<SSPTYPE>***<tab>FICS4=HLRG30<tab> |  |
|  |  | UDS |  | UDSTYPE, MSISDN | **SO\_RCVDATE** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | msisdn=***<MSISDN>***,requestDateTime=***<SO\_RCVDATE>***,accountStatus=ACTIVE,brand=***<UDSTYPE>*** |  |
|  |  | CWS |  | IMSI, MSISDN | **SYSDATE** - format is yyyymmd **SEQNO** - 5-digit, left-padded with zeroes | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | Filename format: ESGF***<SYSDATE>***-***<SEQNO>***.txt File Content:  Header - H<filename><3 spaces><current timestamp yyyyMMddHHmmss>000000<version>0080<24 spaces>  Body - PN9***<IMSI>***<35 spaces>+***<MSISDN>***<14 spaces>  Footer - T<line count of body, 10 digits, left pad with zero><69 spaces> |  |
|  |  | SIACC |  | MSISDN | **SYSDATETIME** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | Filename format: JWP***<SYSDATETIME>*** File Content:  ***<MSISDN>***,ACTIVE |  |
| RFS\_MVOICE | CHGNUMBER\_NC | SSP |  | NEW MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | TXNCODE=GSM\_CHNUM<tab>FICS1=***<MSISDN>***<tab>FICS2=***<NEW MSISDN>***<tab> |  |
|  |  | UDS |  | NEW MSISDN | **SO\_RCVDATE** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | msisdn=***<NEW MSISDN>***,requestDateTime=***<SO\_RCVDATE>***,accountStatus=ACTIVE,brand=***<UDSTYPE>*** |  |
|  |  | APTILO |  | NEW MSISDN |  | 1. Whitelist error code 9001. |  | {"msisdn":"<MSISDN>"} |  |
|  |  | CWS |  | NEW MSISDN, IMSI, MSISDN | **SYSDATE** - format is yyyymmd **SEQNO** - 5-digit, left-padded with zeroes | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | Filename format: ESGF***<SYSDATE>***-***<SEQNO>***.txt File Content:  Header - H<filename><3 spaces><current timestamp yyyyMMddHHmmss>000000<version>0080<24 spaces>  Body - PC9***<IMSI>***<3 spaces>+***<MSISDN>***<19 spaces>+***<NEW MSISDN>***<14 spaces>  Footer - T<line count of body, 10 digits, left pad with zero><69 spaces> |  |
|  |  | MYSMRT |  | NEW MSISDN, MSISDN | **SYSDATETIME** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | Filename format: MyApp\_***<SYSDATETIME>***.txt File Content:  cmin|***<MSISDN>***|***<NEW MSISDN>***|1 |  |
|  |  | SIACC |  | NEW MSISDN | **SYSDATETIME** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | Filename format: JWP***<SYSDATETIME>*** File Content:  ***<MSISDN>***,ACTIVE |  |
| RFS\_MVOICE | RESUME\_NC | SSP |  | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | TXNCODE=GSM\_REACT<tab>FICS1=***<MSISDN>***<tab>FICS2=BALC<tab> |  |
|  |  | UDS |  | MSISDN | **SO\_RCVDATE** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | msisdn=***<MSISDN>***,requestDateTime=***<SO\_RCVDATE>***,accountStatus=ACTIVE,brand=***<UDSTYPE>*** |  |
|  |  | CDP |  | MSISDN | **SO\_RCVDATE** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | <soapenv:Envelope  xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/"  xmlns:ser="http://service.soap.ccengine.mdsp.huawei.com"  xmlns:xsd="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <soapenv:Header/>  <soapenv:Body>  <ser:in0>  <xsd:version>D12x</xsd:version>  <xsd:transactionID>***<SO\_RCVDATE>***</xsd:transactionID>  <xsd:extensionInfo>  <xsd:namedParameters>  <ser:item>  <xsd:key>traceUniqueID</xsd:key>  <xsd:value>504010102231101231715120011002</xsd:value>  </ser:item>  </xsd:namedParameters>  </xsd:extensionInfo>  <xsd:updateType>modify</xsd:updateType>  <xsd:userID>  <xsd:ID>***<MSISDN>***</xsd:ID>  <xsd:type>0</xsd:type>  </xsd:userID>  <xsd:userProfile>  <xsd:payType>0</xsd:payType>  <xsd:userID>  <xsd:ID>***<MSISDN>***</xsd:ID>  <xsd:type>0</xsd:type>  </xsd:userID>  <xsd:userState>0</xsd:userState>  </xsd:userProfile>  </ser:in0>  </soapenv:Body> </soapenv:Envelope> |  |
|  |  | SIACC |  | MSISDN | **SYSDATETIME** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | Filename format: JWP***<SYSDATETIME>*** File Content:  ***<MSISDN>***,ACTIVE |  |
| RFS\_MVOICE | SUSPEND\_NC | SSP |  | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | TXNCODE=GSM\_DEACT<tab>FICS1=***<MSISDN>***<tab>FICS2=BALC<tab> |  |
|  |  | UDS |  | MSISDN | **SO\_RCVDATE** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | msisdn=***<MSISDN>***,requestDateTime=***<SO\_RCVDATE>***,accountStatus=TEMPORARY DISCONNECTED,brand=***<UDSTYPE>*** |  |
|  |  | CDP |  | MSISDN | **SO\_RCVDATE** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | <soapenv:Envelope  xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/"  xmlns:ser="http://service.soap.ccengine.mdsp.huawei.com"  xmlns:xsd="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <soapenv:Header/>  <soapenv:Body>  <ser:in0>  <xsd:version>D12x</xsd:version>  <xsd:transactionID>***<SO\_RCVDATE>***</xsd:transactionID>  <xsd:extensionInfo>  <xsd:namedParameters>  <ser:item>  <xsd:key>traceUniqueID</xsd:key>  <xsd:value>504010102231101231715120011002</xsd:value>  </ser:item>  </xsd:namedParameters>  </xsd:extensionInfo>  <xsd:updateType>modify</xsd:updateType>  <xsd:userID>  <xsd:ID>***<MSISDN>***</xsd:ID>  <xsd:type>0</xsd:type>  </xsd:userID>  <xsd:userProfile>  <xsd:payType>0</xsd:payType>  <xsd:userID>  <xsd:ID>***<MSISDN>***</xsd:ID>  <xsd:type>0</xsd:type>  </xsd:userID>  <xsd:userState>1</xsd:userState>  </xsd:userProfile>  </ser:in0>  </soapenv:Body> </soapenv:Envelope> |  |
|  |  | SIACC |  | MSISDN | **SYSDATETIME** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | Filename format: JWP***<SYSDATETIME>*** File Content:  ***<MSISDN>***,NOT FOUND |  |
| RFS\_MVOICE | REMOVE\_NC | SSP |  | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | TXNCODE=GSM\_DSCON<tab>FICS1=***<MSISDN>***<tab> |  |
|  |  | UDS |  | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | msisdn=***<MSISDN>***,requestDateTime=***<SO\_RCVDATE>***,accountStatus=PERMANENTLY DISCONNECTED,brand=***<UDSTYPE>*** |  |
|  |  | APTILO |  | MSISDN |  | 1. Whitelist error code 9001. |  | {"msisdn":"***<MSISDN>***"} |  |
|  |  | CDP |  | MSISDN | **SO\_RCVDATE** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | <soapenv:Envelope  xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/"  xmlns:ser="http://service.soap.ccengine.mdsp.huawei.com"  xmlns:xsd="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <soapenv:Header/>  <soapenv:Body>  <ser:in0>  <xsd:version>D12x</xsd:version>  <xsd:transactionID>***<SO\_RCVDATE>***</xsd:transactionID>  <xsd:extensionInfo>  <xsd:namedParameters>  <ser:item>  <xsd:key>traceUniqueID</xsd:key>  <xsd:value>504010102231101231715120011002</xsd:value>  </ser:item>  </xsd:namedParameters>  </xsd:extensionInfo>  <xsd:updateType>modify</xsd:updateType>  <xsd:userID>  <xsd:ID>***<MSISDN>***</xsd:ID>  <xsd:type>0</xsd:type>  </xsd:userID>  <xsd:userProfile>  <xsd:payType>0</xsd:payType>  <xsd:userID>  <xsd:ID>***<MSISDN>***</xsd:ID>  <xsd:type>0</xsd:type>  </xsd:userID>  <xsd:userState>9</xsd:userState>  </xsd:userProfile>  </ser:in0>  </soapenv:Body> </soapenv:Envelope> |  |
|  |  | MYSMRT |  | MSISDN | **SYSDATETIME** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | Filename format: MyApp\_***<SYSDATETIME>***.txt File Content:  del|***<MSISDN>***|***<MSISDN>***|1 |  |
|  |  | SIACC |  | MSISDN | **SYSDATETIME** - format is yyyymmddhhmmss | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | Filename format: JWP***<SYSDATETIME>*** File Content:  ***<MSISDN>***,NOT FOUND |  |
| RFS\_IDD | ADD\_NC | SSP |  | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | TXNCODE=GSM\_REACT<tab>FICS1=***<MSISDN>***<tab>FICS2=BIDD<tab> |  |
|  | REMOVE\_NC | SSP |  | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | TXNCODE=GSM\_DEACT<tab>FICS1=***<MSISDN>***<tab>FICS2=BIDD<tab> |  |
|  | RESUME\_NC | SSP |  | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | TXNCODE=GSM\_REACT<tab>FICS1=***<MSISDN>***<tab>FICS2=BIDD<tab> |  |
|  | SUSPEND\_NC | SSP |  | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | TXNCODE=GSM\_DEACT<tab>FICS1=***<MSISDN>***<tab>FICS2=BIDD<tab> |  |
| RFS\_MVOICE | CHGIMSI\_NC | SSP |  | NEW IMSI, IMSI |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | TXNCODE=GSM\_CIMSI<tab>FICS1=<MSISDN><tab>FICS2=<IMSI><tab>FICS3=<NEW IMSI><tab> |  |
|  |  | CWS |  | NEW IMSI |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | Filename format: ESGF<SYSDATE>-<SEQNO>.txt File Content:  Header - H<filename><3 spaces><current timestamp yyyyMMddHHmmss>000000<version>0080<24 spaces>  Body - PP9<IMSI><3 spaces>+<MSISDN>9<NEW IMSI><30 spaces>  Footer - T<line count of body, 10 digits, left pad with zero><69 spaces> |  |
| RFS\_ROAMING | ADD | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=ROAMING\_ADD |  |
| RFS\_ROAMING | REMOVE | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=ROAMING\_REMOVE |  |
| RFS\_ROAMING | SUSPEND | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=ROAMING\_SUSPEND |  |
| RFS\_ROAMING | RESUME | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=ROAMING\_RESUME |  |
| RFS\_BAREINCOMING | ADD | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=BARINCOMING\_ADD |  |
| RFS\_BAREINCOMING | REMOVE | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=BARINCOMING\_REMOVE |  |
| RFS\_BAREINCOMING | RESUME | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=BARINCOMING\_RESUME |  |
| RFS\_BAREINCOMING | SUSPEND | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=BARINCOMING\_SUSPEND |  |
| RFS\_BAROUTGOING | ADD | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=BAROUTGOING\_ADD |  |
| RFS\_BAROUTGOING | REMOVE | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=BAROUTGOING\_REMOVE |  |
| RFS\_BAROUTGOING | RESUME | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=BAROUTGOING\_RESUME |  |
| RFS\_BAROUTGOING | SUSPEND | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=BAROUTGOING\_SUSPEND |  |
| RFS\_CALLHOLD | ADD | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=CALLHOLD\_ADD |  |
| RFS\_CALLHOLD | REMOVE | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=CALLHOLD\_REMOVE |  |
| RFS\_VOLTE | ADD | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI, MSISDN | skiptask |  | USE\_TEMPLATE=VOLTE\_ADD |  |
| RFS\_VOLTE | REMOVE | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=VOLTE\_REMOVE |  |
| RFS\_VOLTE | RESUME | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI, MSISDN | skiptask |  | USE\_TEMPLATE=VOLTE\_RESUME |  |
| RFS\_VOLTE | SUSPEND | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=VOLTE\_SUSPEND |  |
| RFS\_MULTIPARTY | ADD | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=MULTIPARTY\_ADD |  |
| RFS\_MULTIPARTY | REMOVE | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=MULTIPARTY\_REMOVE |  |
| RFS\_DATAROAMING | ADD | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=DATAROAMING\_ADD |  |
| RFS\_DATAROAMING | REMOVE | HLR |  | TS\_HLR\_ONENDS\_V9\_DUMMY | IMSI | skiptask |  | USE\_TEMPLATE=DATAROAMING\_REMOVE |  |
| RFS\_MVOICE | ADD\_NC | ISM |  | TS\_ISM\_SOAP\_V1\_activation | IMSI, MSISDN, ICCID | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | <soapenv:Body>  <web:activation>  <web:activationRequest>  <headerData>  <username><USERNAME></username>  <password><PASSWORD></password>  <transactionId><TRANSACTIONID></transactionId>  </headerData>  <iccid><ICCID></iccid>  <imsi><IMSI></imsi>  <msisdn><MSISDN></msisdn>  </web:activationRequest>  </web:activation> </soapenv:Body> |  |
| RFS\_MVOICE | CHGNUMBER\_NC | ISM |  | TS\_ISM\_SOAP\_V1\_msisdnSwap | MSISDN, NEW\_MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | <soapenv:Body>  <web:msisdnSwap>  <web:msisdnSwapRequest>  <headerData>  <username><USERNAME></username>  <password><PASSWORD></password>  <transactionId><TRANSACTIONID></transactionId>  </headerData>  <oldIccid><ICCID></oldIccid>  <oldMsisdn><MSISDN></oldMsisdn>  <newMsisdn><NEW MSISDN></newMsisdn>  </web:msisdnSwapRequest>  </web:msisdnSwap> </soapenv:Body> |  |
| RFS\_MVOICE | CHGIMSI\_NC | ISM |  | TS\_ISM\_SOAP\_V1\_simSwap | IMSI, NEW\_IMSI | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | <soapenv:Body>  <web:simSwap>  <web:simSwapRequest>  <headerData>  <username><USERNAME></username>  <password><PASSWORD></password>  <transactionId><TRANSACTIONID></transactionId>  </headerData>  <oldImsi><IMSI></oldImsi>  <oldMsisdn><MSISDN></oldMsisdn>  <newImsi><NEW IMSI></newImsi>  </web:simSwapRequest>  </web:simSwap> </soapenv:Body> |  |
| RFS\_MVOICE | REMOVE\_NC | ISM |  | TS\_ISM\_SOAP\_V1\_termination | ICCID | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | <soapenv:Body>  <web:termination>  <web:terminationRequest>  <headerData>  <username><USERNAME></username>  <password><PASSWORD></password>  <transactionId><TRANSACTIONID></transactionId>  </headerData>  <iccid><ICCID></iccid>  <imsi><IMSI></imsi>  <msisdn><MSISDN></msisdn>  </web:terminationRequest>  </web:termination> </soapenv:Body> |  |
| RFS\_MVOICE | ADD\_NC | FMS |  | TS\_FMS\_DB\_CONNECT\_V4\_Create | UDSTYPE | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | fmsdata.p\_so\_insert ('<UDSTYPE>','GSNC','BASIC','NC','','<MSISDN>','','<IMSI>',?); |  |
| RFS\_MVOICE | CHGNUMBER\_NC | FMS |  | TS\_FMS\_DB\_CONNECT\_V4\_ModifyNumber | UDSTYPE, MSISDN, NEW\_MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | fmsdata.p\_so\_insert ('***<UDSTYPE>***','GSCM','CMIN','CMIN','***<MSISDN>***','***<NEW MSISDN>***','','',?); |  |
| RFS\_MVOICE | CHGIMSI\_NC | FMS |  | TS\_FMS\_DB\_CONNECT\_V4\_ModifyIMSI | UDSTYPE, IMSI, NEW\_IMSI | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | fmsdata.p\_so\_insert ('***<UDSTYPE>***','GSCS','CIMSI','CIMSI','','','***<IMSI>***','***<NEW IMSI>***',?); |  |
| RFS\_MVOICE | REMOVE\_NC | FMS |  | TS\_FMS\_DB\_CONNECT\_V4\_REMOVE | UDSTYPE | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS);FAIL POST |  | fmsdata.p\_so\_insert ('***<UDSTYPE>***','GSPD','GSPD','DIS','','***<MSISDN>***','','***<IMSI>***',?); |  |
| RFS\_BAROUTGOING | ADD\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_MOD\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:MOD\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/odbservs/OdbForImsMultimediaTelephonyServices/OutgoingBarring</ats:PATH>  <ats:SERVICEDATA>  <xcap:OutgoingBarring>0</xcap:OutgoingBarring>  </ats:SERVICEDATA>  </ats:MOD\_MSR> </soapenv:Body> |  |
| RFS\_BAROUTGOING | REMOVE\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_RMV\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:RMV\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/odbservs/OdbForImsMultimediaTelephonyServices/OutgoingBarring</ats:PATH>  </ats:RMV\_MSR> </soapenv:Body> |  |
| RFS\_BAROUTGOING | RESUME\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_MOD\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:MOD\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/odbservs/OdbForImsMultimediaTelephonyServices/OutgoingBarring</ats:PATH>  <ats:SERVICEDATA>  <xcap:OutgoingBarring>0</xcap:OutgoingBarring>  </ats:SERVICEDATA>  </ats:MOD\_MSR> </soapenv:Body> |  |
| RFS\_BAROUTGOING | SUSPEND\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_RMV\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:RMV\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/odbservs/OdbForImsMultimediaTelephonyServices/OutgoingBarring</ats:PATH>  </ats:RMV\_MSR> </soapenv:Body> |  |
| RFS\_BARINCOMING | ADD\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_MOD\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:MOD\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/odbservs/OdbForImsMultimediaTelephonyServices/IncomingBarring</ats:PATH>  <ats:SERVICEDATA>  <xcap:IncomingBarring>0</xcap:IncomingBarring>  </ats:SERVICEDATA>  </ats:MOD\_MSR> </soapenv:Body> |  |
| RFS\_BARINCOMING | REMOVE\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_RMV\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:RMV\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/odbservs/OdbForImsMultimediaTelephonyServices/IncomingBarring</ats:PATH>  </ats:RMV\_MSR> </soapenv:Body> |  |
| RFS\_BARINCOMING | RESUME\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_MOD\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:MOD\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/odbservs/OdbForImsMultimediaTelephonyServices/IncomingBarring</ats:PATH>  <ats:SERVICEDATA>  <xcap:IncomingBarring>0</xcap:IncomingBarring>  </ats:SERVICEDATA>  </ats:MOD\_MSR> </soapenv:Body> |  |
| RFS\_BARINCOMING | SUSPEND\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_RMV\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:RMV\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/odbservs/OdbForImsMultimediaTelephonyServices/IncomingBarring</ats:PATH>  </ats:RMV\_MSR> </soapenv:Body> |  |
| RFS\_SMSO | ADD\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_RMV\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:RMV\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/smsservs/complete-short-message/operator-short-message/deactive-send-short-message</ats:PATH>  </ats:RMV\_MSR> </soapenv:Body> |  |
| RFS\_SMSO | REMOVE\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_MOD\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:MOD\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/smsservs/complete-short-message/operator-short-message/deactive-send-short-message</ats:PATH>  <ats:SERVICEDATA>  <xcap:deactive-send-short-message/>  </ats:SERVICEDATA>  </ats:MOD\_MSR> </soapenv:Body> |  |
| RFS\_SMSO | RESUME\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_MOD\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:RMV\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/smsservs/complete-short-message/operator-short-message/deactive-send-short-message</ats:PATH>  </ats:RMV\_MSR> </soapenv:Body> |  |
| RFS\_SMSO | SUSPEND\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_RMV\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:MOD\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/smsservs/complete-short-message/operator-short-message/deactive-send-short-message</ats:PATH>  <ats:SERVICEDATA>  <xcap:deactive-send-short-message/>  </ats:SERVICEDATA>  </ats:MOD\_MSR> </soapenv:Body> |  |
| RFS\_SMST | ADD\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_RMV\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:RMV\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/smsservs/complete-short-message/operator-short-message/deactive-receive-short-message</ats:PATH>  </ats:RMV\_MSR> </soapenv:Body> |  |
| RFS\_SMST | REMOVE\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_MOD\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:MOD\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/smsservs/complete-short-message/operator-short-message/deactive-receive-short-message</ats:PATH>  <ats:SERVICEDATA>  <xcap:deactive-receive-short-message/>  </ats:SERVICEDATA>  </ats:MOD\_MSR> </soapenv:Body> |  |
| RFS\_SMST | RESUME\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_MOD\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:RMV\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/smsservs/complete-short-message/operator-short-message/deactive-receive-short-message</ats:PATH>  </ats:RMV\_MSR> </soapenv:Body> |  |
| RFS\_SMST | SUSPEND\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_RMV\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:MOD\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/smsservs/complete-short-message/operator-short-message/deactive-receive-short-message</ats:PATH>  <ats:SERVICEDATA>  <xcap:deactive-receive-short-message/>  </ats:SERVICEDATA>  </ats:MOD\_MSR> </soapenv:Body> |  |
| RFS\_VOLTE | ADD\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_ADD\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:ADD\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:SERVICEDATA>  <xcap:im-csi-information>  <xcap:supported-imssf-camel-phases>phase3</xcap:supported-imssf-camel-phases>  <xcap:camel-subscription-info/>  </xcap:im-csi-information>  <xcap:MMTel-extension>  <xcap:basic-part>  <xcap:call-source-code>0</xcap:call-source-code>  <xcap:call-out-authority>  <xcap:local>true</xcap:local>  <xcap:local-toll>true</xcap:local-toll>  <xcap:national-toll>true</xcap:national-toll>  <xcap:international-toll>true</xcap:international-toll>  <xcap:intra-local-toll>true</xcap:intra-local-toll>  <xcap:intra-national-toll>true</xcap:intra-national-toll>  <xcap:customized-call-out-authority1>false</xcap:customized-call-out-authority1>  <xcap:customized-call-out-authority2>false</xcap:customized-call-out-authority2>  <xcap:customized-call-out-authority3>false</xcap:customized-call-out-authority3>  <xcap:customized-call-out-authority4>false</xcap:customized-call-out-authority4>  <xcap:customized-call-out-authority5>false</xcap:customized-call-out-authority5>  <xcap:customized-call-out-authority6>false</xcap:customized-call-out-authority6>  <xcap:customized-call-out-authority7>false</xcap:customized-call-out-authority7>  <xcap:customized-call-out-authority8>false</xcap:customized-call-out-authority8>  <xcap:customized-call-out-authority9>false</xcap:customized-call-out-authority9>  <xcap:customized-call-out-authority10>false</xcap:customized-call-out-authority10>  <xcap:customized-call-out-authority11>false</xcap:customized-call-out-authority11>  <xcap:customized-call-out-authority12>false</xcap:customized-call-out-authority12>  <xcap:customized-call-out-authority13>false</xcap:customized-call-out-authority13>  <xcap:customized-call-out-authority14>false</xcap:customized-call-out-authority14>  <xcap:customized-call-out-authority15>false</xcap:customized-call-out-authority15>  <xcap:customized-call-out-authority16>false</xcap:customized-call-out-authority16>  <xcap:customized-call-out-authority17>false</xcap:customized-call-out-authority17>  <xcap:customized-call-out-authority18>false</xcap:customized-call-out-authority18>  <xcap:customized-call-out-authority19>false</xcap:customized-call-out-authority19>  <xcap:customized-call-out-authority20>false</xcap:customized-call-out-authority20>  <xcap:customized-call-out-authority21>false</xcap:customized-call-out-authority21>  <xcap:customized-call-out-authority22>false</xcap:customized-call-out-authority22>  <xcap:customized-call-out-authority23>false</xcap:customized-call-out-authority23>  <xcap:customized-call-out-authority24>false</xcap:customized-call-out-authority24>  <xcap:customized-call-out-authority25>false</xcap:customized-call-out-authority25>  <xcap:customized-call-out-authority26>false</xcap:customized-call-out-authority26>  <xcap:customized-call-out-authority27>false</xcap:customized-call-out-authority27>  <xcap:customized-call-out-authority28>false</xcap:customized-call-out-authority28>  <xcap:customized-call-out-authority29>false</xcap:customized-call-out-authority29>  <xcap:customized-call-out-authority30>false</xcap:customized-call-out-authority30>  <xcap:customized-call-out-authority31>false</xcap:customized-call-out-authority31>  <xcap:customized-call-out-authority32>false</xcap:customized-call-out-authority32>  <xcap:customized-high-entertainment-call-out>false</xcap:customized-high-entertainment-call-out>  <xcap:customized-opertator>false</xcap:customized-opertator>  </xcap:call-out-authority>  <xcap:user-category>ordinary</xcap:user-category>  <xcap:user-password>123456</xcap:user-password>  <xcap:charge-mode>online-charging-and-offline-charging</xcap:charge-mode>  <xcap:limit-group>65534</xcap:limit-group>  <xcap:limitation-of-parallel-calls>1</xcap:limitation-of-parallel-calls>  <xcap:black-white-number-name>test</xcap:black-white-number-name>  <xcap:enhanced-category>10</xcap:enhanced-category>  <xcap:first-level-bill-group>65535</xcap:first-level-bill-group>  <xcap:second-level-bill-group>65535</xcap:second-level-bill-group>  <xcap:video-call-capability>high-definition</xcap:video-call-capability>  <xcap:announcement-set-id>254</xcap:announcement-set-id>  <xcap:bulk-call-flag>0</xcap:bulk-call-flag>  <xcap:enum-sub-domain-index>65535</xcap:enum-sub-domain-index>  <xcap:telephone-number-type>65535</xcap:telephone-number-type>  <xcap:voice-mailbox-address-index>65535</xcap:voice-mailbox-address-index>  <xcap:customized-user-category>0</xcap:customized-user-category>  <xcap:VCC-flag>1</xcap:VCC-flag>  <xcap:conference-group>65535</xcap:conference-group>  <xcap:TV-Notification>0</xcap:TV-Notification>  <xcap:display-index>65534</xcap:display-index>  <xcap:ProvinceID>0</xcap:ProvinceID>  <xcap:limitation-of-parallel-holds>64</xcap:limitation-of-parallel-holds>  <xcap:CS-reroute>0</xcap:CS-reroute>  <xcap:CS-reroute-restriction>0</xcap:CS-reroute-restriction>  <xcap:reserved-field/>  <xcap:reserved-field2>65535</xcap:reserved-field2>  <xcap:reserved-field3>65535</xcap:reserved-field3>  <xcap:reserved-field5>4294967295</xcap:reserved-field5>  <xcap:reserved-field6>4294967295</xcap:reserved-field6>  <xcap:reserved-field7>4294967295</xcap:reserved-field7>  </xcap:basic-part>  </xcap:MMTel-extension>  <xcap:IP-SM-GW>  <xcap:complete-short-message>  <xcap:operator-short-message authorized="true">  <xcap:short-message-preferred-domain>ims-domain</xcap:short-message-preferred-domain>  </xcap:operator-short-message>  </xcap:complete-short-message>  </xcap:IP-SM-GW>  <xcap:OdbForImsOrientedServices>  <xcap:OdbForImsMultimediaTelephonyServices>  <xcap:OutgoingPremiumRateBarring/>  </xcap:OdbForImsMultimediaTelephonyServices>  </xcap:OdbForImsOrientedServices>  </ats:SERVICEDATA>  <ats:TEMPLATENAME><BRAND NAME></ats:TEMPLATENAME>  </ats:ADD\_MSR> </soapenv:Body> |  |
| RFS\_VOLTE | RESUME\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_RMV\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:RMV\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/smsservs/complete-short-message/operator-short-message/deactive-send-short-message</ats:PATH>  </ats:RMV\_MSR> </soapenv:Body> |  |
| RFS\_VOLTE | SUSPEND\_NC | ATS |  | TS\_ATS\_SOAP\_CONNECT\_V1\_MOD\_MSR | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <soapenv:Body>  <ats:MOD\_MSR>  <ats:IMPU>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</ats:IMPU>  <ats:PATH>/smsservs/complete-short-message/operator-short-message/deactive-send-short-message</ats:PATH>  <ats:SERVICEDATA>  <xcap:deactive-send-short-message/>  </ats:SERVICEDATA>  </ats:MOD\_MSR> </soapenv:Body> |  |
| RFS\_IDD | ADD\_NC | FMS |  | TS\_FMS\_DB\_CONNECT\_V4\_Create | UDSTYPE | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | begin fmsdata.p\_so\_insert ('<UDSTYPE>','GSNC','IDD','NC','','<MSISDN>','','<IMSI>',?); end; |  |
| RFS\_ROAMING | ADD\_NC | FMS |  | TS\_FMS\_DB\_CONNECT\_V4\_Create | UDSTYPE | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | begin fmsdata.p\_so\_insert ('<UDSTYPE>','GSNC','IDD','NC','','<MSISDN>','','<IMSI>',?); end; |  |
| RFS\_VOLTE | ADD\_NC | ENUM |  | TS\_ENUM\_SOAP\_CONNECT\_V1\_ADD\_DNAPTRREC | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <SOAP-ENV:Body>  <m:ADD\_DNAPTRREC>  <m:E164NUM><NON63MSISDN></m:E164NUM>  <m:ZONENAME>3.6.e164.arpa</m:ZONENAME>  <m:ORDER>10</m:ORDER>  <m:PREFERENCE>101</m:PREFERENCE>  <m:FLAGS>U</m:FLAGS>  <m:SERVICE>sip+e2u</m:SERVICE>  <m:REGEXP>!^.\*$!sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org!</m:REGEXP>  </m:ADD\_DNAPTRREC> </SOAP-ENV:Body> |  |
| RFS\_VOLTE | REMOVE\_NC | ENUM |  | TS\_ENUM\_SOAP\_CONNECT\_V1\_RMV\_DNAPTRREC | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <SOAP-ENV:Body>  <m:RMV\_DNAPTRREC>  <m:E164NUM><NON63MSISDN></m:E164NUM>  <m:ZONENAME>3.6.e164.arpa</m:ZONENAME>  <m:ENUMFLAG>ENS\_TYPE</m:ENUMFLAG>  </m:RMV\_DNAPTRREC> </SOAP-ENV:Body> |  |
| RFS\_VOLTE | CHGNUMBER\_NC | ENUM |  | TS\_ENUM\_SOAP\_CONNECT\_V1\_RMV\_DNAPTRREC | MSISDN | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST |  | <SOAP-ENV:Body>  <m:RMV\_DNAPTRREC>  <m:E164NUM><NON63MSISDN></m:E164NUM>  <m:ZONENAME>3.6.e164.arpa</m:ZONENAME>  <m:ENUMFLAG>ENS\_TYPE</m:ENUMFLAG>  </m:RMV\_DNAPTRREC> </SOAP-ENV:Body> |  |

|  |  |  |
| --- | --- | --- |
| **<RFS>\_<ACTION>** | **SPML** | **Parameters** |
| BAROUTGOING\_ADD | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>5</status>  </valueObject>  </modification> </request> | IMSI |
| BAROUTGOING\_REMOVE | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | IMSI |
| BAROUTGOING\_RESUME | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>5</status>  </valueObject>  </modification> </request> | IMSI |
| BAROUTGOING\_SUSPEND | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAOC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | IMSI |
| BARINCOMING\_ADD | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>5</status>  </valueObject>  </modification> </request> | IMSI |
| BARINCOMING\_REMOVE | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | IMSI |
| BARINCOMING\_RESUME | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>5</status>  </valueObject>  </modification> </request> | IMSI |
| BARINGCOMING\_SUSPEND | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:BAIC">  <basicServiceGroup>TS10-telephony</basicServiceGroup>  <status>4</status>  </valueObject>  </modification> </request> | IMSI |
| VOLTE\_ADD | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset">  <valueObject xsi:type="subscriber:Subscriber">  <hlr>  <tcsi>  <operatorServiceName>T-CSI6045</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </tcsi>  <smsSubData>  <refPriorityListName>IpSmGw2</refPriorityListName>  </smsSubData>  </hlr>  <hss>  <subscriptionId>1</subscriptionId>  <profileType>normal</profileType>  <adminBlocked>false</adminBlocked>  <defaultScscfRequired>true</defaultScscfRequired>  <privateUserId>  <privateUserId><IMSI>@ims.mnc003.mcc515.3gppnetwork.org</privateUserId>  <provisionedImsi>  <provisionedImsi><IMSI></provisionedImsi>  </provisionedImsi>  <msisdn><MSISDN></msisdn>  <preferredAuthenticationScheme>aka</preferredAuthenticationScheme>  <preferredDomain>none</preferredDomain>  <looseRoutingIndicationRequired>false</looseRoutingIndicationRequired>  </privateUserId>  <privateUserId>  <privateUserId><IMSI>@ics.mnc003.mcc515.3gppnetwork.org</privateUserId>  <provisionedImsi>  <provisionedImsi><IMSI></provisionedImsi>  </provisionedImsi>  <msisdn><MSISDN></msisdn>  <preferredAuthenticationScheme>aka</preferredAuthenticationScheme>  <preferredDomain>none</preferredDomain>  <looseRoutingIndicationRequired>false</looseRoutingIndicationRequired>  </privateUserId>  <implicitRegisteredSet>  <irsId>IRS1</irsId>  <registrationStatus>notRegistered</registrationStatus>  <provisionedPrivateId><IMSI>@ims.mnc003.mcc515.3gppnetwork.org</provisionedPrivateId>  </implicitRegisteredSet>  <publicUserId>  <publicUserId>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</publicUserId>  <originalPublicUserId>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</originalPublicUserId>  <barringIndication>false</barringIndication>  <defaultIndication>true</defaultIndication>  <irsId>IRS1</irsId>  <displayNamePrivacy>false</displayNamePrivacy>  <aliasId>IMPU</aliasId>  <isChildIMPU>false</isChildIMPU>  </publicUserId>  <publicUserId>  <publicUserId>tel:+<MSISDN></publicUserId>  <originalPublicUserId>tel:+<MSISDN></originalPublicUserId>  <barringIndication>false</barringIndication>  <defaultIndication>false</defaultIndication>  <irsId>IRS1</irsId>  <displayNamePrivacy>false</displayNamePrivacy>  <aliasId>IMPU</aliasId>  <isChildIMPU>false</isChildIMPU>  </publicUserId>  <publicUserId>  <publicUserId>sip:<IMSI>@ims.mnc003.mcc515.3gppnetwork.org</publicUserId>  <originalPublicUserId>sip:<IMSI>@ims.mnc003.mcc515.3gppnetwork.org</originalPublicUserId>  <barringIndication>true</barringIndication>  <defaultIndication>false</defaultIndication>  <irsId>IRS1</irsId>  <displayNamePrivacy>false</displayNamePrivacy>  <aliasId>IMPU</aliasId>  <isChildIMPU>false</isChildIMPU>  </publicUserId>  <publicUserId>  <publicUserId>sip:<IMSI>@ics.mnc003.mcc515.3gppnetwork.org</publicUserId>  <originalPublicUserId>sip:<IMSI>@ics.mnc003.mcc515.3gppnetwork.org</originalPublicUserId>  <barringIndication>false</barringIndication>  <defaultIndication>false</defaultIndication>  <irsId>IRS1</irsId>  <displayNamePrivacy>false</displayNamePrivacy>  <aliasId>IMPU</aliasId>  <isChildIMPU>false</isChildIMPU>  </publicUserId>  <serviceProfile>  <profileName>100</profileName>  <mandatoryCapability>  <mandatoryCapability>101</mandatoryCapability>  </mandatoryCapability>  <globalFilterId>  <globalFilterId>107Register</globalFilterId>  </globalFilterId>  <subscribedMediaProfileID>  <sessionReleasePolicy>deregisterNoForcedSessionRelease</sessionReleasePolicy>  <forkingPolicy>noForking</forkingPolicy>  </subscribedMediaProfileID>  </serviceProfile>  <aliasGroup>  <aliasId>IMPU</aliasId>  <serviceProfileName>100</serviceProfileName>  <irsId>IRS1</irsId>  </aliasGroup>  </hss>  </valueObject>  </modification> </request> | IMSI, MSISDN |
| VOLTE\_REMOVE | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hss" operation="remove" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <match xsi:type="subscriber:HSS"/>  </modification>  <modification name="hlr/tcsi" operation="remove" scope="uniqueTypeMapping"/>  <modification name="hlr/smsSubData" operation="remove" scope="uniqueTypeMapping"/> </request> | IMSI |
| VOLTE\_RESUME | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset">  <valueObject xsi:type="subscriber:Subscriber">  <hlr>  <tcsi>  <operatorServiceName>T-CSI6045</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </tcsi>  <smsSubData>  <refPriorityListName>IpSmGw2</refPriorityListName>  </smsSubData>  </hlr>  <hss>  <subscriptionId>1</subscriptionId>  <profileType>normal</profileType>  <adminBlocked>false</adminBlocked>  <defaultScscfRequired>true</defaultScscfRequired>  <privateUserId>  <privateUserId><IMSI>@ims.mnc003.mcc515.3gppnetwork.org</privateUserId>  <provisionedImsi>  <provisionedImsi><IMSI></provisionedImsi>  </provisionedImsi>  <msisdn><MSISDN></msisdn>  <preferredAuthenticationScheme>aka</preferredAuthenticationScheme>  <preferredDomain>none</preferredDomain>  <looseRoutingIndicationRequired>false</looseRoutingIndicationRequired>  </privateUserId>  <privateUserId>  <privateUserId><IMSI>@ics.mnc003.mcc515.3gppnetwork.org</privateUserId>  <provisionedImsi>  <provisionedImsi><IMSI></provisionedImsi>  </provisionedImsi>  <msisdn><MSISDN></msisdn>  <preferredAuthenticationScheme>aka</preferredAuthenticationScheme>  <preferredDomain>none</preferredDomain>  <looseRoutingIndicationRequired>false</looseRoutingIndicationRequired>  </privateUserId>  <implicitRegisteredSet>  <irsId>IRS1</irsId>  <registrationStatus>notRegistered</registrationStatus>  <provisionedPrivateId><IMSI>@ims.mnc003.mcc515.3gppnetwork.org</provisionedPrivateId>  </implicitRegisteredSet>  <publicUserId>  <publicUserId>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</publicUserId>  <originalPublicUserId>sip:+<MSISDN>@ims.mnc003.mcc515.3gppnetwork.org</originalPublicUserId>  <barringIndication>false</barringIndication>  <defaultIndication>true</defaultIndication>  <irsId>IRS1</irsId>  <displayNamePrivacy>false</displayNamePrivacy>  <aliasId>IMPU</aliasId>  <isChildIMPU>false</isChildIMPU>  </publicUserId>  <publicUserId>  <publicUserId>tel:+<MSISDN></publicUserId>  <originalPublicUserId>tel:+<MSISDN></originalPublicUserId>  <barringIndication>false</barringIndication>  <defaultIndication>false</defaultIndication>  <irsId>IRS1</irsId>  <displayNamePrivacy>false</displayNamePrivacy>  <aliasId>IMPU</aliasId>  <isChildIMPU>false</isChildIMPU>  </publicUserId>  <publicUserId>  <publicUserId>sip:<IMSI>@ims.mnc003.mcc515.3gppnetwork.org</publicUserId>  <originalPublicUserId>sip:<IMSI>@ims.mnc003.mcc515.3gppnetwork.org</originalPublicUserId>  <barringIndication>true</barringIndication>  <defaultIndication>false</defaultIndication>  <irsId>IRS1</irsId>  <displayNamePrivacy>false</displayNamePrivacy>  <aliasId>IMPU</aliasId>  <isChildIMPU>false</isChildIMPU>  </publicUserId>  <publicUserId>  <publicUserId>sip:<IMSI>@ics.mnc003.mcc515.3gppnetwork.org</publicUserId>  <originalPublicUserId>sip:<IMSI>@ics.mnc003.mcc515.3gppnetwork.org</originalPublicUserId>  <barringIndication>false</barringIndication>  <defaultIndication>false</defaultIndication>  <irsId>IRS1</irsId>  <displayNamePrivacy>false</displayNamePrivacy>  <aliasId>IMPU</aliasId>  <isChildIMPU>false</isChildIMPU>  </publicUserId>  <serviceProfile>  <profileName>100</profileName>  <mandatoryCapability>  <mandatoryCapability>101</mandatoryCapability>  </mandatoryCapability>  <globalFilterId>  <globalFilterId>107Register</globalFilterId>  </globalFilterId>  <subscribedMediaProfileID>  <sessionReleasePolicy>deregisterNoForcedSessionRelease</sessionReleasePolicy>  <forkingPolicy>noForking</forkingPolicy>  </subscribedMediaProfileID>  </serviceProfile>  <aliasGroup>  <aliasId>IMPU</aliasId>  <serviceProfileName>100</serviceProfileName>  <irsId>IRS1</irsId>  </aliasGroup>  </hss>  </valueObject>  </modification> </request> | IMSI, MSISDN |
| VOLTE\_SUSPEND | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hss" operation="remove" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <match xsi:type="subscriber:HSS"/>  </modification>  <modification name="hlr/tcsi" operation="remove" scope="uniqueTypeMapping"/>  <modification name="hlr/smsSubData" operation="remove" scope="uniqueTypeMapping"/> </request> | IMSI |
| ROAMING\_ADD\_IDC | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <rr>RPI\_all</rr>  <sr>1</sr>  </valueObject>  </modification>  <modification name="hlr/roamSubscription" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:ROAMSUBSCRIPTION">  <roamSubscriptionInfo>PTPD\_DFT10</roamSubscriptionInfo>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSIR1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCIR1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | IMSI |
| ROAMING\_ADD\_CEBU | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <rr>RPI\_all</rr>  <sr>1</sr>  </valueObject>  </modification>  <modification name="hlr/roamSubscription" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:ROAMSUBSCRIPTION">  <roamSubscriptionInfo>PTPD\_DFT10</roamSubscriptionInfo>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSIR1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCIR1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | IMSI |
| ROAMING\_REMOVE\_IDC | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <sr>9</sr>  </valueObject>  </modification>  <modification name="hlr/rr" operation="remove" scope="uniqueTypeMapping"/>  <modification name="hlr/roamSubscription" operation="remove" scope="uniqueTypeMapping"/>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | IMSI |
| ROAMING\_REMOVE\_CEBU | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <sr>9</sr>  </valueObject>  </modification>  <modification name="hlr/rr" operation="remove" scope="uniqueTypeMapping"/>  <modification name="hlr/roamSubscription" operation="remove" scope="uniqueTypeMapping"/>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | IMSI |
| ROAMING\_RESUME\_IDC | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <rr>RPI\_all</rr>  <sr>1</sr>  </valueObject>  </modification>  <modification name="hlr/roamSubscription" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:ROAMSUBSCRIPTION">  <roamSubscriptionInfo>PTPD\_DFT10</roamSubscriptionInfo>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSIR1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCIR1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | IMSI |
| ROAMING\_RESUME\_CEBU | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <rr>RPI\_all</rr>  <sr>1</sr>  </valueObject>  </modification>  <modification name="hlr/roamSubscription" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:ROAMSUBSCRIPTION">  <roamSubscriptionInfo>PTPD\_DFT10</roamSubscriptionInfo>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSIR1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCIR1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | IMSI |
| ROAMING\_SUSPEND\_IDC | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <sr>9</sr>  </valueObject>  </modification>  <modification name="hlr/rr" operation="remove" scope="uniqueTypeMapping"/>  <modification name="hlr/roamSubscription" operation="remove" scope="uniqueTypeMapping"/>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | IMSI |
| ROAMING\_SUSPEND\_CEBU | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="setoradd" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <sr>9</sr>  </valueObject>  </modification>  <modification name="hlr/rr" operation="remove" scope="uniqueTypeMapping"/>  <modification name="hlr/roamSubscription" operation="remove" scope="uniqueTypeMapping"/>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification> </request> | IMSI |
| CALLHOLD\_ADD | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <hold>true</hold>  </valueObject>  </modification> </request> | IMSI |
| CALLHOLD\_REMOVE | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/hold" operation="remove" scope="uniqueTypeMapping"/> </request> | IMSI |
| MULTIPARTY\_ADD | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <mpty>true</mpty>  </valueObject>  </modification> </request> | IMSI |
| MULTIPARTY\_REMOVE | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/mpty" operation="remove" scope="uniqueTypeMapping"/> </request> | IMSI |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| RFS\_FLP | ADD | OCS | TS\_OCS |  | NP\_MSISDN - MSISDN w/o 63-prefixISDN w/o 63-prefix | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <SubActivationRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode> </SubActivationRequest> |  | 1 |  |
| RFS\_FLP | SUBSCRIBE | OCS | TS\_OCS |  | NP\_MSISDN - MSISDN w/o 63-prefixISDN w/o 63-prefix | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <SubActivationRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode> </SubActivationRequest> |  | 1 |  |
|  |  | OCS | TS\_OCS | PRIMARY OFFER ID | NP\_MSISDN - MSISDN w/o 63-prefixISDN w/o 63-prefix | PRE=SKIP THIS TASK IF PRIMARY\_OFFER\_ID is not provided  IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <ChangeSubOfferingRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:PrimaryOffering>  <ns8:NewPrimaryOffering>  <ns7:OfferingKey>  <ns7:OfferingID><PRIMARY OFFER ID></ns7:OfferingID>  </ns7:OfferingKey>  </ns8:NewPrimaryOffering>  <ns8:EffectiveTime>  <ns7:Mode>I</ns7:Mode>  </ns8:EffectiveTime>  </ns8:PrimaryOffering> </ChangeSubOfferingRequest> |  | 2 |  |
|  |  | HLR | TS\_HLR\_ONENDS\_V9\_DUMMY | CHARGING PROFILE, CHARGING BEHAVIOR, ROUTCAT | | SKIPTASK -> CALL LIB\_AGGREGATE | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <mpty>true</mpty>  <rr>RPI\_all</rr>  <sr>1</sr>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <ts21>  <msisdn><MSISDN></msisdn>  </ts21>  <ts22>  <msisdn><MSISDN></msisdn>  </ts22>  <ts61>  <msisdn><MSISDN></msisdn>  </ts61>  <ts62>  <msisdn><MSISDN></msisdn>  </ts62>  <gprs>  <msisdn><MSISDN></msisdn>  </gprs>  <caw/>  <baoc/>  <boic/>  <boicexhc/>  <baic/>  <bicroam/>  <cuss/>  <basicSelfLocation/>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <generalChargingCharacteristics>  <chargingCharacteristicsProfile><CHARGING PROFILE></chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior><CHARGING BEHAVIOR></chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <routingCategory><ROUTCAT></routingCategory>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odboc>2</odboc>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odbr>1</odbr>  </valueObject>  </modification>  <modification name="hlr/cfu" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFU">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfb" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFB">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  <notifyForwardingSubscriber>true</notifyForwardingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfnry" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFNry">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  <notifyForwardingSubscriber>true</notifyForwardingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfnrc" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFNrc">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  </valueObject>  </modification>  <modification name="hlr/emlpp" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EMLPP">  <maxPriority>priority2</maxPriority>  <defaultPriority>priority2</defaultPriority>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>45</id>  <type>2</type>  <qosProfile>SNPOSMB</qosProfile>  <apn>SUNPREPAID</apn>  <apnArea>HPLMN</apnArea>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>45</defaultPdnContextId>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn><MSISDN></msisdn>  </eps>  <epsPdnContext>  <apn>SUNPREPAID</apn>  <contextId>45</contextId>  <type>both</type>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <qos>SunLte</qos>  </epsPdnContext>  </valueObject>  </modification> </request> | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <mpty>true</mpty>  <rr>RPI\_all</rr>  <sr>1</sr>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <ts21>  <msisdn><MSISDN></msisdn>  </ts21>  <ts22>  <msisdn><MSISDN></msisdn>  </ts22>  <ts61>  <msisdn><MSISDN></msisdn>  </ts61>  <ts62>  <msisdn><MSISDN></msisdn>  </ts62>  <gprs>  <msisdn><MSISDN></msisdn>  </gprs>  <caw/>  <baoc/>  <boic/>  <boicexhc/>  <baic/>  <bicroam/>  <cuss/>  <basicSelfLocation/>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <generalChargingCharacteristics>  <chargingCharacteristicsProfile><CHARGING PROFILE></chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior><CHARGING BEHAVIOR></chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <routingCategory><ROUTCAT></routingCategory>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odboc>2</odboc>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odbr>1</odbr>  </valueObject>  </modification>  <modification name="hlr/cfu" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFU">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfb" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFB">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  <notifyForwardingSubscriber>true</notifyForwardingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfnry" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFNry">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  <notifyForwardingSubscriber>true</notifyForwardingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfnrc" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFNrc">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  </valueObject>  </modification>  <modification name="hlr/emlpp" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EMLPP">  <maxPriority>priority2</maxPriority>  <defaultPriority>priority2</defaultPriority>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>45</id>  <type>2</type>  <qosProfile>SNPOSMB</qosProfile>  <apn>SUNPREPAID</apn>  <apnArea>HPLMN</apnArea>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>45</defaultPdnContextId>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn><MSISDN></msisdn>  </eps>  <epsPdnContext>  <apn>SUNPREPAID</apn>  <contextId>45</contextId>  <type>both</type>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <qos>SunLte</qos>  </epsPdnContext>  </valueObject>  </modification> </request> |  |  |
| RFS\_FLP | SUBSCRIBE\_NC | SSP | TS\_SSP\_SEG\_V1\_dscon | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | TXNCODE=GSM\_DSCON<tab>FICS1=<MSISDN><tab> |  |  |  |
|  |  | SSP | TS\_SSP\_SEG\_V1\_preactNWCON | MSISDN, SSPTYPE, IMSI |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | TXNCODE=GSM\_NWCON<tab>FICS1=<MSISDN><tab>FICS2=<IMSI><tab>FICS3=<SSPTYPE><tab>FICS4=HLRG30<tab> |  |  |  |
| RFS\_FLP | CHGIMSI | HLR | TS\_HLR\_ONENDS\_V9\_DUMMY | NEW\_IMSI |  | SKIPTASK -> CALL LIB\_AGGREGATE | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><IMSI></oldId>  <newId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><NEW IMSI></newId> </request> |  |  | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><NEW IMSI></oldId>  <newId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><IMSI></newId> </request> |
|  |  | OCS | TS\_OCS | NEW\_IMSI | NP\_MSISDN - MSISDN w/o 63-prefixISDN w/o 63-prefix | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <ChangeSubIdentityRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:ModifySubIdentity>  <ns8:OldSubIdentity><IMSI></ns8:OldSubIdentity>  <ns8:OldSubIdentityType>2</ns8:OldSubIdentityType>  <ns8:NewSubIdentity><NEW IMSI></ns8:NewSubIdentity>  </ns8:ModifySubIdentity> </ChangeSubIdentityRequest> |  |  | <ChangeSubIdentityRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:ModifySubIdentity>  <ns8:OldSubIdentity><NEW IMSI></ns8:OldSubIdentity>  <ns8:OldSubIdentityType>2</ns8:OldSubIdentityType>  <ns8:NewSubIdentity><IMSI></ns8:NewSubIdentity>  </ns8:ModifySubIdentity> </ChangeSubIdentityRequest> |
| RFS\_FLP | CHGIMSI\_NC | SSP | TS\_SSP\_SEG\_V1\_cimsi | NEW\_IMSI |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | TXNCODE=GSM\_CIMSI<tab>FICS1=<MSISDN><tab>FICS2=<IMSI><tab>FICS3=<NEW IMSI><tab> |  |  |  |
|  |  | ISM | TS\_ISM\_SOAP\_V1\_simSwap | NEW\_IMSI |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <soapenv:Body>  <web:simSwap>  <web:simSwapRequest>  <headerData>  <username><USERNAME></username>  <password><PASSWORD></password>  <transactionId><TRANSACTIONID></transactionId>  </headerData>  <oldImsi><IMSI></oldImsi>  <oldMsisdn><MSISDN></oldMsisdn>  <newImsi><NEW IMSI></newImsi>  </web:simSwapRequest>  </web:simSwap> </soapenv:Body> |  |  |  |
| RFS\_FLP | CHGNUMBER | HLR | TS\_HLR\_ONENDS\_V9\_DUMMY | NEW\_MSISDN |  | SKIPTASK -> CALL LIB\_AGGREGATE | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><MSISDN></oldId>  <newId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><NEW MSISDN></newId> </request> |  |  | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><NEW MSISDN></oldId>  <newId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><MSISDN></newId> </request> |
|  |  | OCS | TS\_OCS | NEW\_MSISDN | NP\_MSISDN - MSISDN w/o 63-prefixISDN w/o 63-prefix NP\_NEW\_MSISDN - NEW\_MSISDN w/o 63-prefixISDN w/o 63-prefix | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <ChangeSubIdentityRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:ModifySubIdentity>  <ns8:OldSubIdentity><NON63MSISDN></ns8:OldSubIdentity>  <ns8:OldSubIdentityType>1</ns8:OldSubIdentityType>  <ns8:NewSubIdentity><NEW NON63MSISDN></ns8:NewSubIdentity>  </ns8:ModifySubIdentity> </ChangeSubIdentityRequest> |  | 1 | <ChangeSubIdentityRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NEW NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:ModifySubIdentity>  <ns8:OldSubIdentity><NEW NON63MSISDN></ns8:OldSubIdentity>  <ns8:OldSubIdentityType>1</ns8:OldSubIdentityType>  <ns8:NewSubIdentity><NON63MSISDN></ns8:NewSubIdentity>  </ns8:ModifySubIdentity> </ChangeSubIdentityRequest> |
|  |  | vUPCC | TS\_PCRF\_UPCC | NEW\_MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <ns2:updateSubscriber  xmlns:ns2="rm:soap">  <inPara>  <subscriber>  <attribute>  <key>usrIdentifier</key>  <value><NEW MSISDN></value>  </attribute>  <attribute>  <key>oldusrIdentifier</key>  <value><MSISDN></value>  </attribute>  </subscriber>  </inPara> </ns2:updateSubscriber> |  | 1 | <ns2:updateSubscriber  xmlns:ns2="rm:soap">  <inPara>  <subscriber>  <attribute>  <key>usrIdentifier</key>  <value><MSISDN></value>  </attribute>  <attribute>  <key>oldusrIdentifier</key>  <value><NEW MSISDN></value>  </attribute>  </subscriber>  </inPara> </ns2:updateSubscriber> |
| RFS\_FLP | CHGNUMBER\_NC | SSP | TS\_SSP\_SEG\_V1\_chnum | NEW MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | TXNCODE=GSM\_CHNUM<tab>FICS1=<MSISDN><tab>FICS2=<NEW MSISDN><tab> |  |  |  |
|  |  | ISM | TS\_ISM\_SOAP\_V1\_msisdnSwap | NEW MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <soapenv:Body>  <web:msisdnSwap>  <web:msisdnSwapRequest>  <headerData>  <username><USERNAME></username>  <password><PASSWORD></password>  <transactionId><TRANSACTIONID></transactionId>  </headerData>  <oldIccid><ICCID></oldIccid>  <oldMsisdn><MSISDN></oldMsisdn>  <newMsisdn><NEW MSISDN></newMsisdn>  </web:msisdnSwapRequest>  </web:msisdnSwap> </soapenv:Body> |  |  |  |
| RFS\_FLP | UNSUBSCRIBE | HLR | TS\_HLR\_ONENDS\_V9\_DUMMY |  |  | SKIPTASK -> CALL LIB\_AGGREGATE | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <mpty>false</mpty>  <rr>RPI\_all</rr>  <sr>1</sr>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <ts21>  <msisdn><MSISDN></msisdn>  </ts21>  <ts22>  <msisdn><MSISDN></msisdn>  </ts22>  <ts61>  <msisdn><MSISDN></msisdn>  </ts61>  <ts62>  <msisdn><MSISDN></msisdn>  </ts62>  <gprs>  <msisdn><MSISDN></msisdn>  </gprs>  <caw/>  <baoc/>  <boic/>  <boicexhc/>  <baic/>  <bicroam/>  <cuss/>  <basicSelfLocation/>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <generalChargingCharacteristics>  <chargingCharacteristicsProfile>4</chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior>7</chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <routingCategory>100</routingCategory>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odbr>1</odbr>  </valueObject>  </modification>  <modification name="hlr/emlpp" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EMLPP">  <maxPriority>priority4</maxPriority>  <defaultPriority>priority4</defaultPriority>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>45</id>  <type>2</type>  <qosProfile>SNPREMB</qosProfile>  <apn>SUNPREPAID</apn>  <apnArea>HPLMN</apnArea>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>45</defaultPdnContextId>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn><MSISDN></msisdn>  </eps>  <epsPdnContext>  <apn>SUNPREPAID</apn>  <contextId>45</contextId>  <type>both</type>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <qos>SunLte</qos>  </epsPdnContext>  </valueObject>  </modification> </request> | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <mpty>false</mpty>  <rr>RPI\_all</rr>  <sr>1</sr>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <ts21>  <msisdn><MSISDN></msisdn>  </ts21>  <ts22>  <msisdn><MSISDN></msisdn>  </ts22>  <ts61>  <msisdn><MSISDN></msisdn>  </ts61>  <ts62>  <msisdn><MSISDN></msisdn>  </ts62>  <gprs>  <msisdn><MSISDN></msisdn>  </gprs>  <caw/>  <baoc/>  <boic/>  <boicexhc/>  <baic/>  <bicroam/>  <cuss/>  <basicSelfLocation/>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <generalChargingCharacteristics>  <chargingCharacteristicsProfile>4</chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior>7</chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <routingCategory>100</routingCategory>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odbr>1</odbr>  </valueObject>  </modification>  <modification name="hlr/emlpp" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EMLPP">  <maxPriority>priority4</maxPriority>  <defaultPriority>priority4</defaultPriority>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>45</id>  <type>2</type>  <qosProfile>SNPREMB</qosProfile>  <apn>SUNPREPAID</apn>  <apnArea>HPLMN</apnArea>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>45</defaultPdnContextId>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn><MSISDN></msisdn>  </eps>  <epsPdnContext>  <apn>SUNPREPAID</apn>  <contextId>45</contextId>  <type>both</type>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <qos>SunLte</qos>  </epsPdnContext>  </valueObject>  </modification> </request> |  |  |
| RFS\_FLP | UNSUBSCRIBE\_NC | SSP | TS\_SSP\_SEG\_V1\_dscon | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | TXNCODE=GSM\_DSCON<tab>FICS1=***<MSISDN>***<tab> |  |  |  |
|  |  | SSP | TS\_SSP\_SEG\_V1\_preactNWCON | MSISDN, SSPTYPE, IMSI |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | TXNCODE=GSM\_NWCON<tab>FICS1=<MSISDN><tab>FICS2=<IMSI><tab>FICS3=277<tab>FICS4=HLRG30<tab> |  |  |  |
| RFS\_FLP | REMOVE | HLR | TS\_HLR\_ONENDS\_V9\_DUMMY |  |  | SKIPTASK -> CALL LIB\_AGGREGATE | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/>  <modification name="auc" operation="remove"/> </request> |  |  |  |
|  | REMOVE | OCS | TS\_OCS |  | NP\_MSISDN - MSISDN w/o 63-prefixISDN w/o 63-prefix | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <ChangeSubOfferingRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:PrimaryOffering>  <ns8:NewPrimaryOffering>  <ns7:OfferingKey>  <ns7:OfferingID>800000</ns7:OfferingID>  </ns7:OfferingKey>  </ns8:NewPrimaryOffering>  <ns8:EffectiveTime>  <ns7:Mode>I</ns7:Mode>  </ns8:EffectiveTime>  </ns8:PrimaryOffering> </ChangeSubOfferingRequest> |  |  |  |
|  |  | vUPCC | TS\_PCRF\_UPCC |  |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <ns2:delSubscriber  xmlns:ns2="rm:soap">  <inPara>  <subscriber>  <attribute>  <key>usrIdentifier</key>  <value><MSISDN></value>  </attribute>  </subscriber>  </inPara> </ns2:delSubscriber> |  |  |  |
|  |  | DP9 | TS\_DP9\_SOAP\_V1\_deleteSubscription |  |  | POST IF FAILED - CALL DP9\_HANDLING and RESEND  IF FAILED AGAIN MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) | <soapenv:Envelope  xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/"  xmlns:xsd="http://www.w3.org/2001/XMLSchema"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <soapenv:Body>  <deleteSubscription  xmlns="http://smarttrust.com.repository.subscriptionmodule">  <identifier xmlns="">  <identifier><IMSI></identifier>  <type>IMSI</type>  </identifier>  </deleteSubscription>  </soapenv:Body> </soapenv:Envelope> |  | 1 |  |
|  |  |  | TS\_DP9\_SOAP\_V1\_deleteCard | ICCID |  | POST IF FAILED - CALL DP9\_HANDLING and RESEND  IF FAILED AGAIN MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) | <soapenv:Envelope  xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/"  xmlns:xsd="http://www.w3.org/2001/XMLSchema"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <soapenv:Body>  <deleteCard  xmlns="http://smarttrust.com.repository.cardmodule">  <iccid xmlns=""><ICCID></iccid>  </deleteCard>  </soapenv:Body> </soapenv:Envelope> |  | 1 |  |
| RFS\_FLP | REMOVE\_NC | SSP | TS\_SSP\_SEG\_V1\_dscon | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | TXNCODE=GSM\_DSCON<tab>FICS1=<MSISDN><tab> |  |  |  |
|  |  | ISM | TS\_ISM\_SOAP\_V1\_termination | MSISDN,IMSI |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <soapenv:Body>  <web:termination>  <web:terminationRequest>  <headerData>  <username><USERNAME></username>  <password><PASSWORD></password>  <transactionId><TRANSACTIONID></transactionId>  </headerData>  <iccid><ICCID></iccid>  <imsi><IMSI></imsi>  <msisdn><MSISDN></msisdn>  </web:terminationRequest>  </web:termination> </soapenv:Body> |  |  |  |
|  |  | UREG | TS\_SOAP\_CONNECT\_V1\_UREG\_PurgeMIN | MSISDN |  | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:ws="http://ws.register.smart.com/">  <soapenv:Header/>  <soapenv:Body>  <ws:purgeMin>  <ANumber>(MANDATORY\_MSISDN1)</ANumber>  <Channel>(MANDATORY\_CHANNEL\_ID)</Channel>  </ws:purgeMin>  </soapenv:Body> </soapenv:Envelope> |  |  |  |
| RFS\_FLP | RESUME | OCS | TS\_OCS |  | NP\_MSISDN - MSISDN w/o 63-prefixISDN w/o 63-prefix | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <ChangeSubStatusRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>30</ns8:OpType> </ChangeSubStatusRequest> |  |  | <ChangeSubStatusRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>32</ns8:OpType> </ChangeSubStatusRequest> |
| RFS\_FLP | SUSPEND | OCS | TS\_OCS |  | NP\_MSISDN - MSISDN w/o 63-prefixISDN w/o 63-prefix | IFNOTEQUAL(%SO<n>\_STATUS,7) MAP(TASK\_NE\_ID\_<n>=($ISM\_NE\_ID),RFS\_CODE\_<n>=%SO<n>\_TECHNICALPRODUCT,TASK\_ERROR\_CODE\_<n>=%SO<n>\_SMESSAGE\_ID,TASK\_ERROR\_MSG\_<n>=%SO<n>\_SMESSAGE\_CAUSE,REQ\_FINAL\_STATUS\_<n>=%SO<n>\_STATUS) POST | <ChangeSubStatusRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>32</ns8:OpType> </ChangeSubStatusRequest> |  |  | <ChangeSubStatusRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>30</ns8:OpType> </ChangeSubStatusRequest> |

|  |  |  |
| --- | --- | --- |
| **<RFS>\_<ACTION>** | **SPML** | **Parameters** |
| FLP\_ADD\_IDC | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <mpty>true</mpty>  <rr>RPI\_all</rr>  <sr>1</sr>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <ts21>  <msisdn><MSISDN></msisdn>  </ts21>  <ts22>  <msisdn><MSISDN></msisdn>  </ts22>  <ts61>  <msisdn><MSISDN></msisdn>  </ts61>  <ts62>  <msisdn><MSISDN></msisdn>  </ts62>  <gprs>  <msisdn><MSISDN></msisdn>  </gprs>  <caw/>  <baoc/>  <boic/>  <boicexhc/>  <baic/>  <bicroam/>  <cuss/>  <basicSelfLocation/>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <generalChargingCharacteristics>  <chargingCharacteristicsProfile><CHARGING PROFILE></chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior><CHARGING BEHAVIOR></chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <routingCategory><ROUTCAT></routingCategory>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odboc>2</odboc>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odbr>1</odbr>  </valueObject>  </modification>  <modification name="hlr/cfu" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFU">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfb" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFB">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  <notifyForwardingSubscriber>true</notifyForwardingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfnry" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFNry">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  <notifyForwardingSubscriber>true</notifyForwardingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfnrc" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFNrc">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  </valueObject>  </modification>  <modification name="hlr/emlpp" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EMLPP">  <maxPriority>priority2</maxPriority>  <defaultPriority>priority2</defaultPriority>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>45</id>  <type>2</type>  <qosProfile>SNPOSMB</qosProfile>  <apn>SUNPREPAID</apn>  <apnArea>HPLMN</apnArea>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>45</defaultPdnContextId>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn><MSISDN></msisdn>  </eps>  <epsPdnContext>  <apn>SUNPREPAID</apn>  <contextId>45</contextId>  <type>both</type>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <qos>SunLte</qos>  </epsPdnContext>  </valueObject>  </modification> </request> | IMSI, MSISDN, CHARGING PROFILE, CHARGING BEHAVIOR, ROUTCAT |
| FLP\_ADD\_CEBU | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <mpty>true</mpty>  <rr>RPI\_all</rr>  <sr>1</sr>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <ts21>  <msisdn><MSISDN></msisdn>  </ts21>  <ts22>  <msisdn><MSISDN></msisdn>  </ts22>  <ts61>  <msisdn><MSISDN></msisdn>  </ts61>  <ts62>  <msisdn><MSISDN></msisdn>  </ts62>  <gprs>  <msisdn><MSISDN></msisdn>  </gprs>  <caw/>  <baoc/>  <boic/>  <boicexhc/>  <baic/>  <bicroam/>  <cuss/>  <basicSelfLocation/>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <generalChargingCharacteristics>  <chargingCharacteristicsProfile><CHARGING PROFILE></chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior><CHARGING BEHAVIOR></chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <routingCategory><ROUTCAT></routingCategory>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odboc>2</odboc>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odbr>1</odbr>  </valueObject>  </modification>  <modification name="hlr/cfu" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFU">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfb" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFB">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  <notifyForwardingSubscriber>true</notifyForwardingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfnry" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFNry">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  <notifyForwardingSubscriber>true</notifyForwardingSubscriber>  </valueObject>  </modification>  <modification name="hlr/cfnrc" operation="add" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:CFNrc">  <notifyCallingSubscriber>true</notifyCallingSubscriber>  </valueObject>  </modification>  <modification name="hlr/emlpp" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EMLPP">  <maxPriority>priority2</maxPriority>  <defaultPriority>priority2</defaultPriority>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>45</id>  <type>2</type>  <qosProfile>SNPOSMB</qosProfile>  <apn>SUNPREPAID</apn>  <apnArea>HPLMN</apnArea>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>45</defaultPdnContextId>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn><MSISDN></msisdn>  </eps>  <epsPdnContext>  <apn>SUNPREPAID</apn>  <contextId>45</contextId>  <type>both</type>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <qos>SunLte</qos>  </epsPdnContext>  </valueObject>  </modification> </request> | IMSI, MSISDN, CHARGING PROFILE, CHARGING BEHAVIOR, ROUTCAT |
| FLP\_CHGIMSI | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><IMSI></oldId>  <newId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><NEW IMSI></newId> </request> | IMSI, MSISDN, NEW\_IMSI |
| FLP\_CHGNUMBER | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><MSISDN></oldId>  <newId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><NEW MSISDN></newId> </request> | IMSI, MSISDN, NEW\_MSISDN |
| FLP\_UNSUBSCRIBE\_IDC | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <mpty>false</mpty>  <rr>RPI\_all</rr>  <sr>1</sr>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <ts21>  <msisdn><MSISDN></msisdn>  </ts21>  <ts22>  <msisdn><MSISDN></msisdn>  </ts22>  <ts61>  <msisdn><MSISDN></msisdn>  </ts61>  <ts62>  <msisdn><MSISDN></msisdn>  </ts62>  <gprs>  <msisdn><MSISDN></msisdn>  </gprs>  <caw/>  <baoc/>  <boic/>  <boicexhc/>  <baic/>  <bicroam/>  <cuss/>  <basicSelfLocation/>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <generalChargingCharacteristics>  <chargingCharacteristicsProfile>4</chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior>7</chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <routingCategory>100</routingCategory>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odbr>1</odbr>  </valueObject>  </modification>  <modification name="hlr/emlpp" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EMLPP">  <maxPriority>priority4</maxPriority>  <defaultPriority>priority4</defaultPriority>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>45</id>  <type>2</type>  <qosProfile>SNPREMB</qosProfile>  <apn>SUNPREPAID</apn>  <apnArea>HPLMN</apnArea>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>45</defaultPdnContextId>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn><MSISDN></msisdn>  </eps>  <epsPdnContext>  <apn>SUNPREPAID</apn>  <contextId>45</contextId>  <type>both</type>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <qos>SunLte</qos>  </epsPdnContext>  </valueObject>  </modification> </request> | IMSI, MSISDN |
| FLP\_UNSUBSCRIBE\_CEBU | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <mpty>false</mpty>  <rr>RPI\_all</rr>  <sr>1</sr>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <ts21>  <msisdn><MSISDN></msisdn>  </ts21>  <ts22>  <msisdn><MSISDN></msisdn>  </ts22>  <ts61>  <msisdn><MSISDN></msisdn>  </ts61>  <ts62>  <msisdn><MSISDN></msisdn>  </ts62>  <gprs>  <msisdn><MSISDN></msisdn>  </gprs>  <caw/>  <baoc/>  <boic/>  <boicexhc/>  <baic/>  <bicroam/>  <cuss/>  <basicSelfLocation/>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <generalChargingCharacteristics>  <chargingCharacteristicsProfile>4</chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior>7</chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <routingCategory>100</routingCategory>  </valueObject>  </modification>  <modification name="hlr" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:HLR">  <odbr>1</odbr>  </valueObject>  </modification>  <modification name="hlr/emlpp" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EMLPP">  <maxPriority>priority4</maxPriority>  <defaultPriority>priority4</defaultPriority>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>45</id>  <type>2</type>  <qosProfile>SNPREMB</qosProfile>  <apn>SUNPREPAID</apn>  <apnArea>HPLMN</apnArea>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>45</defaultPdnContextId>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn><MSISDN></msisdn>  </eps>  <epsPdnContext>  <apn>SUNPREPAID</apn>  <contextId>45</contextId>  <type>both</type>  <maxBandwidthUp>250000000</maxBandwidthUp>  <maxBandwidthDown>500000000</maxBandwidthDown>  <qos>SunLte</qos>  </epsPdnContext>  </valueObject>  </modification> </request> | IMSI, MSISDN |
| FLP\_REMOVE | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/>  <modification name="auc" operation="remove"/> </request> | IMSI |
| FLP\_CHGIMSI\_RB | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><NEW IMSI></oldId>  <newId alias="imsi" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLRSwapIdentifier"><IMSI></newId> </request> | IMSI, MSISDN, NEW\_IMSI |
| FLP\_CHGNUMBER\_RB | <request xsi:type="spml:ChangeIdRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <oldId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><NEW MSISDN></oldId>  <newId alias="msisdn" xsi:type="subscriber:HLRSwapIdentifier"><MSISDN></newId> </request> | IMSI, MSISDN, NEW\_MSISDN |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Catalog item** | **Transaction** | **NETWORK ELEMENT** | **Technical Service** | **Parameters** | **Parameters/Attributes Internal to USPS** | **ACTIONCODE/CONDITION** | **Expected command** | **Sequence command** | **UNDO Transaction** |
| RFS\_IPTVCUSTOMER | ADD | CIGNAL | TS\_CIGNAL\_IPTV\_V1\_CreateCustomer | ORDERNO ACCOUNT\_NUMBER OPERATIONALENTITY CATEGORY  CUSTOMERTYPE SALESCODE |  | IF SUCCESS, MAP IPTV\_CUSTOMER\_NO=@NEW@CUSTOMER\_NO | POST <address1>/customer/createcustomer HTTP/1.1 Content-type: application/json  Accept: application/json Body:  {  "referenceNumber": "<ORDERNO>",  "operationalEntity": "<OPERATIONALENTITY>",  "category": "<CATEGORY>",  "customerType": "<CUSTOMERTYPE>",  "salesCode": "<SALESCODE>",  "nplay": "<ACCOUNT\_NUMBER>",  "firstName": "<ACCOUNT\_NUMBER>",  "lastName": "<ACCOUNT\_NUMBER>"  "country": "PHILIPPINES",  "region": "NCR",  "superRegion": "LUZON",  "province": "METRO MANILA",  "municipality": "MAKATI CITY",  "barangay": "PASEO DE ROXAS",  "address": "PLDT",  "zipCode": "1226" } |  |  |
|  | CHGOWNERSHIP | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_CreateTicket | ORDERNO CUSTOMERNUMBER |  |  | ASSIGNED\_TO=teamcrm CALL\_ID=PFBR($OrderNo) CATEGORY\_ID=2 CLASSIFICATION\_ID=1 CREATOR=pfbr\_appuser CUSTOMER\_ID=($customernumber) DESCRIPTION=RFS:($SO($SO\_IDX)\_TECHNICALPRODUCT)\_ACTION:($SO($SO\_IDX)\_ACTIONCODE)\_OPERATIONALENTITY:($SO($SO\_IDX)\_OPERATIONALENTITY) LAST\_ACT\_DURATION=1 PASSWORD=P1dt0x45 PRIORITY\_ID=2 SERVICE\_ID=1 SOURCE\_ID=31 STATUS\_ID=open TITLE=Account Modification USER\_NAME=pldtfbr | 1 |  |
|  |  | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_GetTicket |  |  | IF @NEW@STATUS\_ID equals open, call LIB\_SERVICEDESQ\_GETTICKET\_RESEND  IF LIB\_STATUS is FAILED, FAILSO | PASSWORD=P1dt0x45 TICKET\_ID=($@NEW\_TICKET\_ID) TYPE=incident USER\_NAME=pldtfbr | 2 |  |
| RFS\_IPTVPPV | ADD | CIGNAL | TS\_CIGNAL\_IPTV\_V1\_AddSubscription | ORDERNO ISSUINGENTITY CUSTOMERNUMBER PLANCODE | STB\_SN1 STB\_SC\_SN1 STB\_SN2 STB\_SC\_SN2 STB\_SN3 STB\_SC\_SN3 | IF SUCCESS, MAP PPV\_CONTRACT\_NO=@NEW@CONTRACT\_NO | POST <address1>/subscription/addsubscription HTTP/1.1 Content-type: application/json  Accept: application/json Body:  {  "referenceNumber": "<ORDERNO>",  " issuingEntity": "<ISSUINGENTITY>",  "customerNumber": "<CUSTOMERNUMBER>",  "planCode": "<PLANCODE>",  "stbBoxSerial": "<STB\_SN1>",  "smartCardSerial": "<STB\_SC\_SN1>",  "stbBoxSerial2": "<STB\_SN2>",  "smartCardSerial2": "<STB\_SC\_SN2>",  "stbBoxSerial3": "<STB\_SN3>",  "smartCardSerial3": "<STB\_SC\_SN3>", } |  |  |
|  | REMOVE | CIGNAL | TS\_CIGNAL\_IPTV\_V1\_DisconSubscription | ORDERNO CONTRACTNO |  |  | POST <address1>/subscription/disconnectsubscription HTTP/1.1 Content-type: application/json  Accept: application/json Body:  {  "referenceNumber": "<REFERENCE\_NUMBER>",  "contractNumber": "<CONTRACTNO>",  "reason": "NOPAY",  "remarks": "",  "disconnectionDate": "<PPV\_DISCONNECTION\_DATE>", } |  |  |
| RFS\_SATTVCUSTOMER | ADD | CIGNAL | TS\_CIGNAL\_IPTV\_V1\_CreateCustomer | ORDERNO OPERATIONALENTITY CATEGORY  CUSTOMERTYPE SALESCODE |  |  | POST <address1>/customer/createcustomer HTTP/1.1 Content-type: application/json  Accept: application/json Body:  {  "referenceNumber": "<ORDERNO>",  "operationalEntity": "<OPERATIONALENTITY>",  "category": "<CATEGORY>",  "customerType": "<CUSTOMERTYPE>",  "salesCode": "<SALESCODE>",  "nplay": "<ACCOUNT\_NUMBER>",  "firstName": "<FIRSTNAME>",  "lastName": "<LASTNAME>",  "country": "PHILIPPINES",  "region": "NCR",  "superRegion": "LUZON",  "province": "METRO MANILA",  "municipality": "MAKATI CITY",  "barangay": "PASEO DE ROXAS",  "address": "PLDT",  "zipCode": "1226" } | 1 |  |
| RFS\_SATTV | ADD | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_CreateTicket | ORDERNO CUSTOMERNUMBER |  |  | ASSIGNED\_TO=teamactivations CALL\_ID=PFBR($OrderNo) CATEGORY\_ID=5 CLASSIFICATION\_ID=1 CREATOR=pfbr\_appuser CUSTOMER\_ID=($customernumber) DESCRIPTION=RFS:($SO($SO\_IDX)\_TECHNICALPRODUCT)\_ACTION:($SO($SO\_IDX)\_ACTIONCODE)\_PLANCODE:($SO($SO\_IDX)\_PLANCODE)\_ISSUINGENTITY:($SO($SO\_IDX)\_ISSUINGENTITY) LAST\_ACT\_DURATION=1 PASSWORD=P1dt0x45 PRIORITY\_ID=3 SERVICE\_ID=3 SOURCE\_ID=31 STATUS\_ID=open TITLE=Activation USER\_NAME=pldtfbr | 2 |  |
|  |  | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_GetTicket |  |  | IF @NEW@STATUS\_ID equals open, call LIB\_SERVICEDESQ\_GETTICKET\_RESEND  IF LIB\_STATUS is FAILED, FAILSO | PASSWORD=P1dt0x45 TICKET\_ID=($@NEW\_TICKET\_ID) TYPE=incident USER\_NAME=pldtfbr | 2 |  |
|  | REMOVE | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_CreateTicket | ORDERNO CUSTOMERNUMBER |  |  | ASSIGNED\_TO=teamcollections CALL\_ID=PFBR($OrderNo) CATEGORY\_ID=712 CLASSIFICATION\_ID=1 CREATOR=pfbr\_appuser CUSTOMER\_ID=($customernumber) DESCRIPTION=DESCRIPTION=RFS:($SO($SO\_IDX)\_TECHNICALPRODUCT)\_ACTION:($SO($SO\_IDX)\_ACTIONCODE) LAST\_ACT\_DURATION=1 PASSWORD=P1dt0x45 PRIORITY\_ID=3 SERVICE\_ID=2 SOURCE\_ID=31 STATUS\_ID=open TITLE=Disconnection USER\_NAME=pldtfbr | 2 |  |
|  |  | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_GetTicket |  |  | IF @NEW@STATUS\_ID equals open, call LIB\_SERVICEDESQ\_GETTICKET\_RESEND  IF LIB\_STATUS is FAILED, FAILSO | PASSWORD=P1dt0x45 TICKET\_ID=($@NEW\_TICKET\_ID) TYPE=incident USER\_NAME=pldtfbr | 2 |  |
|  | CHGPLAN | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_CreateTicket | ORDERNO CUSTOMERNUMBER |  |  | ASSIGNED\_TO=teamcrm CALL\_ID=PFBR($OrderNo) CATEGORY\_ID=55 CLASSIFICATION\_ID=1 CREATOR=pfbr\_appuser CUSTOMER\_ID=($customernumber) DESCRIPTION=RFS:($SO($SO\_IDX)\_TECHNICALPRODUCT)\_ACTION:($SO($SO\_IDX)\_ACTIONCODE)\_PLANCODE:($SO($SO\_IDX)\_PLANCODE)\_OLDPLANCODE:($SO($SO\_IDX)\_OLDPLANCODE) LAST\_ACT\_DURATION=1 PASSWORD=P1dt0x45 PRIORITY\_ID=2 SERVICE\_ID=10 SOURCE\_ID=31 STATUS\_ID=open TITLE=Change Plan USER\_NAME=pldtfbr | 2 |  |
|  |  | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_GetTicket |  |  | IF @NEW@STATUS\_ID equals open, call LIB\_SERVICEDESQ\_GETTICKET\_RESEND  IF LIB\_STATUS is FAILED, FAILSO | PASSWORD=P1dt0x45 TICKET\_ID=($@NEW\_TICKET\_ID) TYPE=incident USER\_NAME=pldtfbr | 2 |  |
|  | SUSPEND | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_CreateTicket | ORDERNO CUSTOMERNUMBER |  |  | ASSIGNED\_TO=teamcollections CALL\_ID=PFBR($OrderNo) CATEGORY\_ID=712 CLASSIFICATION\_ID=1 CREATOR=pfbr\_appuser CUSTOMER\_ID=($customernumber) DESCRIPTION=RFS:($SO($SO\_IDX)\_TECHNICALPRODUCT)\_ACTION:($SO($SO\_IDX)\_ACTIONCODE)\_PLANCODE:($SO($SO\_IDX)\_PLANCODE) LAST\_ACT\_DURATION=1 PASSWORD=P1dt0x45 PRIORITY\_ID=3 SERVICE\_ID=2 SOURCE\_ID=31 STATUS\_ID=open TITLE=Disconnection USER\_NAME=pldtfbr | 2 |  |
|  |  | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_GetTicket |  |  | IF @NEW@STATUS\_ID equals open, call LIB\_SERVICEDESQ\_GETTICKET\_RESEND  IF LIB\_STATUS is FAILED, FAILSO | PASSWORD=P1dt0x45 TICKET\_ID=($@NEW\_TICKET\_ID) TYPE=incident USER\_NAME=pldtfbr | 2 |  |
|  | RESUME | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_CreateTicket | ORDERNO CUSTOMERNUMBER |  |  | ASSIGNED\_TO=teamcollections CALL\_ID=PFBR($OrderNo) CATEGORY\_ID=713 CLASSIFICATION\_ID=1 CREATOR=pfbr\_appuser CUSTOMER\_ID=($customernumber) DESCRIPTION=RFS:($SO($SO\_IDX)\_TECHNICALPRODUCT)\_ACTION:($SO($SO\_IDX)\_ACTIONCODE)\_PLANCODE:($SO($SO\_IDX)\_PLANCODE) LAST\_ACT\_DURATION=1 PASSWORD=P1dt0x45 PRIORITY\_ID=3 SERVICE\_ID=2 SOURCE\_ID=31 STATUS\_ID=open TITLE=Reconnection USER\_NAME=pldtfbr | 2 |  |
|  |  | SERVICEDESQ | TS\_SERVICE\_DESQ\_V1\_GetTicket |  |  | IF @NEW@STATUS\_ID equals open, call LIB\_SERVICEDESQ\_GETTICKET\_RESEND  IF LIB\_STATUS is FAILED, FAILSO | PASSWORD=P1dt0x45 TICKET\_ID=($@NEW\_TICKET\_ID) TYPE=incident USER\_NAME=pldtfbr | 2 |  |
| RFS\_STB | ADD | CIGNAL | TS\_CIGNAL\_IPTV\_V1\_AddSubscription |  |  | SKIPTASK |  |  |  |
| RFS\_PVR | ADD | CIGNAL | TS\_CIGNAL\_IPTV\_V1\_AddSubscription |  |  | SKIPTASK |  |  |  |
| RFS\_VOIP | ND | ISM | TS\_ISM\_SOAP\_V1\_getNumberDetail | TELEPHONE |  | MAP INQ\_SOFTXIP=ACUDETAIL.IPADDRESS INQ\_LDN=LDN INQ\_FINSET=SWEETVOICE |  |  |  |
|  |  | N2000 | TS\_UMS\_N2000\_V300R010C05\_modUser | TELEPHONE | INQ\_SOFTXIP INQ\_LDNSET INQ\_FINSET  Note: This will be generated via and Inquire from ISM getNumberDetails |  | MOD-USR:TID:SOFTXIP="**<INQ\_SOFTXIP>**":<CTAG>::D="**<TELEPHONE>**",LP="**<INQ\_LDNSET>**",CSC="**<INQ\_FINSET>**"; |  |  |
|  |  | OCS | TS\_OCS\_HUAWEI\_V500R005C60LG0022\_createSubscriberSWEETVOICE | ACCOUNT\_NUMBER |  |  | <?xml version="1.0" encoding="utf-8"?><soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/"><soapenv:Header></soapenv:Header><soapenv:Body><ns4:CreateSubscriberRequestMsg xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices" xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon" xmlns:ns4="http://www.huawei.com/bme/cbsinterface/bcservices" xmlns:ns3="http://www.huawei.com/bme/cbsinterface/bccommon" xmlns:ns2="http://www.huawei.com/bme/cbsinterface/cbscommon"><RequestHeader><ns2:Version>1</ns2:Version><ns2:MessageSeq>2019-09-10T01:08:37.835204946768728935562</ns2:MessageSeq><ns2:OwnershipInfo><ns2:BEID>102</ns2:BEID></ns2:OwnershipInfo><ns2:AccessSecurity><ns2:LoginSystemCode>Sweetvoice</ns2:LoginSystemCode><ns2:Password>FLHtrhSvJ73fof26OJ7i/shitttJhNy+JxAjpW3IS6U=</ns2:Password></ns2:AccessSecurity><ns2:OperatorInfo><ns2:OperatorID>102</ns2:OperatorID></ns2:OperatorInfo><ns2:TimeFormat><ns2:TimeType>1</ns2:TimeType></ns2:TimeFormat></RequestHeader><CreateSubscriberRequest><ns4:RegisterCustomer OpType="1"><ns4:CustKey><ACCOUNT NUMBER></ns4:CustKey></ns4:RegisterCustomer><ns4:Account><ns4:AcctKey><ACCOUNT NUMBER></ns4:AcctKey><ns4:AcctInfo><ns3:AcctCode><ACCOUNT NUMBER></ns3:AcctCode><ns3:PaymentType>1</ns3:PaymentType></ns4:AcctInfo></ns4:Account><ns4:Subscriber><ns4:SubscriberKey><ACCOUNT NUMBER></ns4:SubscriberKey><ns4:SubscriberInfo><ns3:SubBasicInfo><ns3:SubProperty><ns3:Code>C\_N\_OVERDUE\_AMT</ns3:Code><ns3:Value>10000</ns3:Value></ns3:SubProperty><ns3:SubProperty><ns3:Code>C\_N\_MO\_LOCAL\_CALL</ns3:Code><ns3:Value>0</ns3:Value></ns3:SubProperty><ns3:SubProperty><ns3:Code>C\_N\_MO\_NDD\_CALL</ns3:Code><ns3:Value>0</ns3:Value></ns3:SubProperty><ns3:SubProperty><ns3:Code>C\_N\_MO\_IDD\_CALL</ns3:Code><ns3:Value>0</ns3:Value></ns3:SubProperty><ns3:SubProperty><ns3:Code>C\_N\_MO\_OPERATOR\_CALL</ns3:Code><ns3:Value>0</ns3:Value></ns3:SubProperty><ns3:SubProperty><ns3:Code>C\_N\_MT\_LOCAL\_CALL</ns3:Code><ns3:Value>0</ns3:Value></ns3:SubProperty><ns3:SubProperty><ns3:Code>C\_N\_MT\_NONLOCAL\_CALL</ns3:Code><ns3:Value>1</ns3:Value></ns3:SubProperty><ns3:SubProperty><ns3:Code>C\_N\_SPECIAL\_CALL</ns3:Code><ns3:Value>0</ns3:Value></ns3:SubProperty></ns3:SubBasicInfo><ns3:UserCustomerKey><ACCOUNT NUMBER></ns3:UserCustomerKey><ns3:SubIdentity><ns3:SubIdentityType>1</ns3:SubIdentityType><ns3:SubIdentity><ACCOUNT NUMBER></ns3:SubIdentity><ns3:PrimaryFlag>1</ns3:PrimaryFlag></ns3:SubIdentity><ns3:Status>2</ns3:Status></ns4:SubscriberInfo><ns4:SubPaymentMode><ns4:PaymentMode>1</ns4:PaymentMode><ns4:AcctKey><ACCOUNT NUMBER></ns4:AcctKey></ns4:SubPaymentMode></ns4:Subscriber><ns4:PrimaryOffering><ns3:OfferingKey><ns3:OfferingID>500014</ns3:OfferingID></ns3:OfferingKey></ns4:PrimaryOffering></CreateSubscriberRequest></ns4:CreateSubscriberRequestMsg></soapenv:Body></soapenv:Envelope> | 1 |  |
|  |  | OCS | TS\_OCS\_HUAWEI\_V500R005C60LG0022\_changeSubStatus | ACCOUNT\_NUMBER |  |  | <?xml version="1.0" encoding="utf-8"?><soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/"><soapenv:Header></soapenv:Header><soapenv:Body><ns4:ChangeSubStatusRequestMsg xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices" xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon" xmlns:ns4="http://www.huawei.com/bme/cbsinterface/bcservices" xmlns:ns3="http://www.huawei.com/bme/cbsinterface/bccommon" xmlns:ns2="http://www.huawei.com/bme/cbsinterface/cbscommon"><RequestHeader><ns2:Version>1</ns2:Version><ns2:MessageSeq>2019-09-10T01:08:38.289156882262228935562</ns2:MessageSeq><ns2:OwnershipInfo><ns2:BEID>102</ns2:BEID></ns2:OwnershipInfo><ns2:AccessSecurity><ns2:LoginSystemCode>Sweetvoice</ns2:LoginSystemCode><ns2:Password>FLHtrhSvJ73fof26OJ7i/shitttJhNy+JxAjpW3IS6U=</ns2:Password></ns2:AccessSecurity><ns2:OperatorInfo><ns2:OperatorID>102</ns2:OperatorID></ns2:OperatorInfo><ns2:TimeFormat><ns2:TimeType>1</ns2:TimeType></ns2:TimeFormat></RequestHeader><ChangeSubStatusRequest><ns4:SubAccessCode><ns3:PrimaryIdentity><ACCOUNT NUMBER></ns3:PrimaryIdentity></ns4:SubAccessCode><ns4:OpType>61</ns4:OpType></ChangeSubStatusRequest></ns4:ChangeSubStatusRequestMsg></soapenv:Body></soapenv:Envelope> | 2 |  |
| RFS\_VOIP | NDLIFT | ISM | TS\_ISM\_SOAP\_V1\_getNumberDetail | TELEPHONE |  | MAP INQ\_SOFTXIP=ACUDETAIL.IPADDRESS INQ\_LDN=LDN INQ\_FINSET=SWEETVOICE |  |  |  |
|  |  | N2000 | TS\_UMS\_N2000\_V300R010C05\_modUser | TELEPHONE | INQ\_SOFTXIP INQ\_LDNSET INQ\_FINSET  Note: This will be generated via and Inquire from ISM getNumberDetails |  | MOD-USR:TID:SOFTXIP="**<INQ\_SOFTXIP>**":<CTAG>::D="**<TELEPHONE>**",LP="**<INQ\_LDNSET>**",CSC="**<INQ\_FINSET>**"; |  |  |
|  |  | OCS | TS\_OCS\_HUAWEI\_V500R005C60LG0022\_subDeactivation | ACCOUNT\_NUMBER |  |  | <?xml version="1.0" encoding="utf-8"?><soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/"><soapenv:Header></soapenv:Header><soapenv:Body><ns4:SubDeactivationRequestMsg xmlns:ns6="http://www.huawei.com/bme/cbsinterface/bbservices" xmlns:ns5="http://www.huawei.com/bme/cbsinterface/bbcommon" xmlns:ns4="http://www.huawei.com/bme/cbsinterface/bcservices" xmlns:ns3="http://www.huawei.com/bme/cbsinterface/bccommon" xmlns:ns2="http://www.huawei.com/bme/cbsinterface/cbscommon"><RequestHeader><ns2:Version>1</ns2:Version><ns2:MessageSeq>2019-09-10T01:11:11.430123012668428935562</ns2:MessageSeq><ns2:OwnershipInfo><ns2:BEID>102</ns2:BEID></ns2:OwnershipInfo><ns2:AccessSecurity><ns2:LoginSystemCode>Sweetvoice</ns2:LoginSystemCode><ns2:Password>FLHtrhSvJ73fof26OJ7i/shitttJhNy+JxAjpW3IS6U=</ns2:Password></ns2:AccessSecurity><ns2:OperatorInfo><ns2:OperatorID>102</ns2:OperatorID></ns2:OperatorInfo><ns2:TimeFormat><ns2:TimeType>1</ns2:TimeType></ns2:TimeFormat></RequestHeader><SubDeactivationRequest><ns4:SubAccessCode><ns3:PrimaryIdentity><ACCOUNT NUMBER></ns3:PrimaryIdentity></ns4:SubAccessCode><ns4:OpType>3</ns4:OpType></SubDeactivationRequest></ns4:SubDeactivationRequestMsg></soapenv:Body></soapenv:Envelope> | 3 |  |
| RFS\_DSL | ND | SAPC SDB | TS\_SDB\_BRIDGEWATER\_98\_getUser |  | INQ\_OPTION82 Note: This will be retrieved via inquire from ARM. Still pending from customer |  | <request version="3.7" principal="admin" credentials="admin"><target name="UserAPI" operation="getUser"><parameter><user><login-name>**<INQ\_OPTION82>**</login-name><profile-set/></user></parameter></target></request> | 1 |  |
|  |  | SAPC SDB | TS\_SDB\_BRIDGEWATER\_98\_updateUser |  | INQ\_OPTION82 Note: This will be retrieved via inquire from ARM. Still pending from customer |  | <request version="3.7" principal="admin" credentials="admin"><target name="UserAPI" operation="updateUser"><parameter><user><login-name>**<INQ\_OPTION82>**</login-name><profile-set><data-subscription-profile><selected-service-components><service-component><qualified-name>/SC\_NoticeDisconnection</qualified-name></service-component></selected-service-components></data-subscription-profile></profile-set></user></parameter></target></request> | 2 |  |
| RFS\_DSL | NDLIFT | SAPC SDB | TS\_SDB\_BRIDGEWATER\_98\_getUser |  | INQ\_OPTION82 Note: This will be retrieved via inquire from ARM. Still pending from customer |  | <request version="3.7" principal="admin" credentials="admin"><target name="UserAPI" operation="getUser"><parameter><user><login-name>**<INQ\_OPTION82>**</login-name><profile-set/></user></parameter></target></request> | 1 |  |
|  |  | SAPC SDB | TS\_SDB\_BRIDGEWATER\_98\_updateUser |  | INQ\_OPTION82 Note: This will be retrieved via inquire from ARM. Still pending from customer |  | <request version="3.7" principal="admin" credentials="admin"><target name="UserAPI" operation="updateUser"><parameter><user><login-name>**<INQ\_OPTION82>**</login-name><profile-set><data-subscription-profile><selected-service-components><service-component delete="true"><qualified-name>/SC\_Redirect</qualified-name></service-component><service-component delete="true"><qualified-name>/SC\_FTTH</qualified-name></service-component></selected-service-components></data-subscription-profile></profile-set></user></parameter></target></request> | 2 |  |
|  |  | SAPC SDB | TS\_SDB\_BRIDGEWATER\_98\_updateUser |  | INQ\_OPTION82 Note: This will be retrieved via inquire from ARM. Still pending from customer |  | <request version="3.7" principal="admin" credentials="admin"><target name="UserAPI" operation="updateUser"><parameter><user><login-name>**<INQ\_OPTION82>**</login-name><profile-set><data-subscription-profile><selected-service-components><service-component delete="true"><qualified-name>/SC\_NoticeDisconnection</qualified-name></service-component></selected-service-components></data-subscription-profile></profile-set></user></parameter></target></request> | 3 |  |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Catalog item** | **Transaction** | **NETWORK ELEMENT** | **Technical Service** | **Parameters** | **Parameters/Attributes Internal to USPS** | **ACTIONCODE/CONDITION** | **Expected command** | **Sequence command** | **UNDO Transaction** |
| RFS\_MVOICE\_INTRA | ADD | OOCS | TS\_OCS\_HUAWEI\_V500R005C60LG0022\_createCustomer | PRIMARY ACCOUNT, ACCOUNT NUMBER, BILL CUTOFF DAY, PRIMARY OFFER ID |  | PRE=IFEQUAL(HLR\_CAMPUS,CEBU), skip  PRE=if PRIMARY ACCOUNT is set to 'N', no need to execute 1st command  POST exec IF error, Generate parameters: NEID\_1,RFS\_1,ERROR\_CODE\_1,ERROR\_MSG\_1 via Map command   POST exec IF Error FAIL SO | <CreateCustomerRequest>  <ns8:RegisterCustKey><ACCOUNT NUMBER></ns8:RegisterCustKey>  <ns8:Customer>  <ns8:CustKey><ACCOUNT NUMBER></ns8:CustKey>  <ns8:CustInfo>  <ns7:CustClass>1</ns7:CustClass>  <ns7:CustCode><ACCOUNT NUMBER></ns7:CustCode>  <ns7:CustBasicInfo>  <ns7:CustProperty>  <ns7:Code>C\_MSISDN\_FOR\_ROUTE</ns7:Code>  <ns7:Value><NON63MSISDN></ns7:Value>  </ns7:CustProperty>  </ns7:CustBasicInfo>  </ns8:CustInfo>  </ns8:Customer>  <ns8:DFTAccount>  <ns8:PayRelationKey><ACCOUNT NUMBER></ns8:PayRelationKey>  <ns8:AcctKey><ACCOUNT NUMBER></ns8:AcctKey>  <ns8:AcctInfo>  <ns7:AcctCode><ACCOUNT NUMBER></ns7:AcctCode>  <ns7:BillCycleType><BILL CUTOFF DAY></ns7:BillCycleType>  <ns7:AcctType>1</ns7:AcctType>  <ns7:PaymentType>1</ns7:PaymentType>  <ns7:AcctClass>1</ns7:AcctClass>  <ns7:CurrencyID>1117</ns7:CurrencyID>  <ns7:InitBalance>0</ns7:InitBalance>  <ns7:AcctPayMethod>1</ns7:AcctPayMethod>  </ns8:AcctInfo>  </ns8:DFTAccount> </CreateCustomerRequest> | 1a | <SubDeactivationRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>3</ns8:OpType> </SubDeactivationRequest> |
| RFS\_MVOICE\_INTRA | ADD | OOCS | TS\_OCS\_HUAWEI\_V500R005C60LG0022\_createSubscriber | PRIMARY ACCOUNT, ACCOUNT NUMBER, BILL CUTOFF DAY, PRIMARY OFFER ID |  | PRE=IFEQUAL(HLR\_CAMPUS,CEBU), skip  PRE=if PRIMARY ACCOUNT is set to 'N', no need to execute 1st command  POST exec IF error, Generate parameters: NEID\_1,RFS\_1,ERROR\_CODE\_1,ERROR\_MSG\_1 via Map command   POST exec IF Error FAIL SO | <CreateSubscriberRequest>  <ns8:RegisterCustomer OpType="2">  <ns8:CustKey><ACCOUNT NUMBER></ns8:CustKey>  </ns8:RegisterCustomer>  <ns8:Subscriber>  <ns8:SubscriberKey><SUBSCRIBER KEY></ns8:SubscriberKey>  <ns8:SubscriberInfo>  <ns7:UserCustomerKey><ACCOUNT NUMBER></ns7:UserCustomerKey>  <ns7:SubIdentity>  <ns7:SubIdentityType>1</ns7:SubIdentityType>  <ns7:SubIdentity><NON63MSISDN></ns7:SubIdentity>  <ns7:PrimaryFlag>1</ns7:PrimaryFlag>  </ns7:SubIdentity>  <ns7:SubClass>2</ns7:SubClass>  <ns7:Status>2</ns7:Status>  </ns8:SubscriberInfo>  <ns8:SubPaymentMode>  <ns8:PaymentMode>1</ns8:PaymentMode>  <ns8:PayRelationKey><SUBSCRIBER KEY></ns8:PayRelationKey>  <ns8:AcctKey><ACCOUNT NUMBER></ns8:AcctKey>  </ns8:SubPaymentMode>  </ns8:Subscriber>  <ns8:PrimaryOffering>  <ns7:OfferingKey>  <ns7:OfferingID><PRIMARY OFFER ID></ns7:OfferingID>  </ns7:OfferingKey>  </ns8:PrimaryOffering> </CreateSubscriberRequest> | 1b | <CustDeactivationRequest>  <ns8:CustAccessCode>  <ns7:CustomerKey><ACCOUNT NUMBER></ns7:CustomerKey>  </ns8:CustAccessCode>  <ns8:OpType>2</ns8:OpType> </CustDeactivationRequest> |
| RFS\_MVOICE\_INTRA | ADD | HLR | TS\_HLR\_ONENDS\_V9\_DUMMY | USE\_TEMPLATE=MVOICE\_INTRA\_ADD |  |  | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <imsiActive>true</imsiActive>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <sr>9</sr>  <ts11>  <msisdn><MSISDN></msisdn>  </ts11>  <bs20genr>  <msisdn><MSISDN></msisdn>  </bs20genr>  <bs30genr>  <msisdn><MSISDN></msisdn>  </bs30genr>  <gprs>  <msisdn><MSISDN></msisdn>  </gprs>  <cuss>  <status>2</status>  </cuss>  <basicSelfLocation>  <status>2</status>  </basicSelfLocation>  <optimalRouting>true</optimalRouting>  <ndcLac><NDCLAC></ndcLac>  <generalChargingCharacteristics>  <chargingCharacteristicsProfile><CHARGING PROFILE></chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior><CHARGING BEHAVIOR></chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  <supportNewRadioSecondaryRAT>true</supportNewRadioSecondaryRAT>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <odboc>2</odboc>  <odbic>0</odbic>  <odboprc>0</odboprc>  <odbssm>0</odbssm>  <odbsci>0</odbsci>  </valueObject>  </modification>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <odbgprs>2</odbgprs>  </valueObject>  </modification> </request> | 2 |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | ISM | TS\_ISM\_SOAP\_V1\_changeBrand | MSISDN1=($MSISDN) BRAND\_CODE=($SUB\_BRAND) |  |  | <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:web="http://web.external.ism.eai.mt.com/">  <soapenv:Header/>  <soapenv:Body>  <web:changeBrand>  <web:changeBrandRequest>  <headerData>  <username>wsuser</username>  <password>abcdefg123456</password>  <transactionId></transactionId>  </headerData>  <iccid></iccid>  <imsi></imsi>  <msisdn>MSISDN</msisdn>  <brandCode>Brand (need to tranlate to ISM Brand) </brandCode>  <subBrand>subrand (need to translate to ISM Brand) </subBrand>  <remarks></remarks>  </web:changeBrandRequest>  </web:changeBrand>  </soapenv:Body> </soapenv:Envelope> | 1a |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | ISM | TS\_ISM\_SOAP\_V1\_changeBillingCycle | MSISDN1=($MSISDN) BILLING\_TYPE=($ISM\_BILLING\_TYPE) |  | Pre-Execution: MAP(ISM\_BILLING\_TYPE=($ACCOUNT\_TYPE)),STR\_UPPER(ISM\_BILLING\_TYPE) | <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:web="http://web.external.ism.eai.mt.com/">  <soapenv:Header/>  <soapenv:Body>  <web:changeBillingType>  <web:changeBillingTypeRequest>  <headerData>  <username>wsuser</username>  <password> abcdefg123456</password>  <transactionId>1234</transactionId>  </headerData>  <iccid></iccid>  <imsi></imsi>  <msisdn>MSISDN</msisdn>  <billingType>account\_type</billingType>  <remarks></remarks>  </web:changeBillingTypeRequest>  </web:changeBillingType>  </soapenv:Body> </soapenv:Envelope> | 1b |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | CDP | TS\_CDP\_XML\_V1\_SYNCUSERDATA | PAY\_TYPE=($CDP\_PAY\_TYPE) USER\_BRAND=($ROUTCAT) USERID\_TYPE=0 |  | Pre-Execution: IF $ACCOUNT\_TYPE==Postpaid MAP CDP\_PAY\_TYPE=0 ELSEIF $ACCOUNT\_TYPE==Prepaid MAP CDP\_PAY\_TYPE=1 | POST /bme/services/SISService HTTP/1.1 Content-Length: 5438 Content-Type: text/xml;charset=utf-8 SOAPAction: "" User-Agent: Java/1.6.0\_10-rc2 Host: 10.137.213.127:21322 Accept: text/html, image/gif, image/jpeg, \*; q=.2, \*/\*; q=.2 Connection: keep-alive  <?xml version="1.0" encoding="utf-8"?> <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:xsd="http://www.w3.org/2001/XMLSchema" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"> <soapenv:Header>  <ns1:IBSoapHeader soapenv:actor="http://schemas.xmlsoap.org/soap/actor/next" soapenv:mustUnderstand="0" xmlns:ns1="http://soapheader.ib.sdp.huawei.com">  <ns1:version>V1.0</ns1:version>  <ns1:traceUniqueID>000000102651206180843180001001</ns1:traceUniqueID>  <ns1:sourceDeviceType>23</ns1:sourceDeviceType>  <ns1:sourceDeviceCode>2300000001</ns1:sourceDeviceCode>  <ns1:destDeviceType>0</ns1:destDeviceType>  <ns1:destDeviceCode>0000000001</ns1:destDeviceCode> <ns1:authenticatorSource>9d32d1185baa0883d9fd9c86ffeed7e92c38fd4770265f2a8e09466294a0c502</ns1:authenticatorSource>  <ns1:timeStamp>20191014162246</ns1:timeStamp>  </ns1:IBSoapHeader> </soapenv:Header>  <soapenv:Body>  <in0 xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <extensionInfo xmlns="http://struct.soap.ccengine.mdsp.huawei.com">  <namedParameters xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <item xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <key xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">who am I?</key>  <value xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">WWWW</value>  </item>  </namedParameters>  </extensionInfo>  <version xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">V1.0</version>  <transactionID xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">OrderNO</transactionID>  <updateType xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">Modify</updateType>  <userID xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <ID>MSISDN</ID>  <type>0</type>  </userID>  <userProfile xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <extensionInfo xmlns="http://struct.soap.ccengine.mdsp.huawei.com">  <namedParameters xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <item xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <key xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">isRoam</key>  <value xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">1</value>  </item>  </namedParameters>  </extensionInfo>  <userName>fine</userName>  <payType>account\_type ( 0 Postpaid 1 prepaid) </payType> <userBrand> routecat from Optima </userBrand>  <userID>  <ID>MSISDN</ID>  <type>0</type>  </userID>  <userState>0</userState>  <userType>0</userType>  <userSID>12345</userSID>  </userProfile>  </in0>  </soapenv:Body> </soapenv:Envelope> | 1c |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | AGW | TS\_AGW\_SOAP\_V1\_SYNCUSERDATA | PAY\_TYPE=($AGW\_PAY\_TYPE) USER\_BRAND=($ROUTCAT) |  | Pre-Execution: IF $ACCOUNT\_TYPE==Postpaid MAP AGW\_PAY\_TYPE=0 ELSEIF $ACCOUNT\_TYPE==Prepaid MAP AGW\_PAY\_TYPE=1 | POST /bme/services/SISService HTTP/1.1 Content-Length: 5438 Content-Type: text/xml;charset=utf-8 SOAPAction: "" User-Agent: Java/1.6.0\_10-rc2 Host: 10.137.213.127:21322 Accept: text/html, image/gif, image/jpeg, \*; q=.2, \*/\*; q=.2 Connection: keep-alive  <?xml version="1.0" encoding="utf-8"?> <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:xsd="http://www.w3.org/2001/XMLSchema" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"> <soapenv:Header>  <ns1:IBSoapHeader soapenv:actor="http://schemas.xmlsoap.org/soap/actor/next" soapenv:mustUnderstand="0" xmlns:ns1="http://soapheader.ib.sdp.huawei.com">  <ns1:version>V1.0</ns1:version>  <ns1:traceUniqueID>000000102651206180843180001001</ns1:traceUniqueID>  <ns1:sourceDeviceType>23</ns1:sourceDeviceType>  <ns1:sourceDeviceCode>2300000001</ns1:sourceDeviceCode>  <ns1:destDeviceType>0</ns1:destDeviceType>  <ns1:destDeviceCode>0000000001</ns1:destDeviceCode> <ns1:authenticatorSource>9d32d1185baa0883d9fd9c86ffeed7e92c38fd4770265f2a8e09466294a0c502</ns1:authenticatorSource>  <ns1:timeStamp>20191014162246</ns1:timeStamp>  </ns1:IBSoapHeader> </soapenv:Header>  <soapenv:Body>  <in0 xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <extensionInfo xmlns="http://struct.soap.ccengine.mdsp.huawei.com">  <namedParameters xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <item xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <key xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">who am I?</key>  <value xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">WWWW</value>  </item>  </namedParameters>  </extensionInfo>  <version xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">V1.0</version>  <transactionID xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">OrderNO</transactionID>  <updateType xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">Modify</updateType>  <userID xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <ID>MSISDN</ID>  <type>0</type>  </userID>  <userProfile xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <extensionInfo xmlns="http://struct.soap.ccengine.mdsp.huawei.com">  <namedParameters xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <item xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <key xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">isRoam</key>  <value xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">1</value>  </item>  </namedParameters>  </extensionInfo>  <userName>fine</userName>  <payType>account\_type ( 0 Postpaid 1 prepaid) </payType>  <userID>  <ID>MSISDN</ID>  <type>7</type>  </userID>  <userState>0</userState>  <userType>0</userType>  <userSID>12345</userSID>  </userProfile>  </in0>  </soapenv:Body> </soapenv:Envelope> | 1d |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | OTA | TS\_OTA\_OPENAPI\_V1\_get | HTTP\_REQUEST\_MSISDN=($MSISDN) | HTTP\_REQUEST\_ACCESS\_CODE=($BST\_ACCESS\_CODE) HTTP\_REQUEST\_KWD=($BST\_KEYWORD) HTTP\_REQUEST\_SVCID=($BST\_SERVICE\_ID) | Post-Execution: If error\_code == 0005 || 9999 SET MNP\_OTA\_ERROR\_FILE = TRUE |  | 1e |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | OTA\_FILE | TS\_FILE\_FORMATPARSER\_ANY\_ota\_file | REQ\_TYPE=1 OPER\_TYPE=MNP\_OTA ACTION=MNP\_OTA MSISDN=($MSISDN) |  | Pre-Execution: If MNP\_OTA\_ERROR\_FILE ParamExist && MNP\_OTA\_ERROR\_FILE == TRUE, executeTask Else skiptask |  |  |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | MPCC | TS\_MPCC\_FILE\_V1\_CreateMpcc | MSISDN=($MSISDN) BRAND=($BRAND) TYPE=($ACCOUNT\_TYPE) |  |  | <MSISDN>|<BRAND>|<TYPE>|<REFERENCE ID> | 1f |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | CWS | TS\_CWS\_SOAP\_V1\_SIMCHANGEBRAND | newSimType=($SIMTYPE\_($SUB\_BRAND)) newPrepaidIndicator=($CWS\_ACCOUNT\_TYPE) |  | Pre-Execution: IF ($ACCOUNT\_TYPE)=='Postpaid' MAP CWS\_ACCOUNT\_TYPE='POST\_PAID' IF ($ACCOUNT\_TYPE)=='Prepaid' MAP CWS\_ACCOUNT\_TYPE='PREPAID' Post-Execution IF ($ERROR\_CODE)=='D067001' IGNOREFAIL, MAP EXEC\_CWS\_SIMPROVISIONING=TRUE | <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:sim="http://smart.com.ph/SimProv">  <soapenv:Header/>  <soapenv:Body>  <sim:SIMChangeBrandRequest>  <msisdn><MSISDN></msisdn>  <oldSimType><OLDSIMTYPE></oldSimType>  <newSimType><NEWSIMTYPE></newSimType>  <oldPrepaidIndicator><OLDPREPAIDINDICATOR></oldPrepaidIndicator>  <newPrepaidIndicator><NEWPREPAIDINDICATOR></newPrepaidIndicator>  </sim:SIMChangeBrandRequest>  </soapenv:Body> </soapenv:Envelope> | 1g |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | ISM | TS\_ISM\_SOAP\_V1\_getSimInfo | IMSI=($IMSI) |  | Pre-Execution: IFNOTEXIST(EXEC\_CWS\_SIMPROVISIONING), SKIPTASK Post-Execution: ISM\_ICCID=<ICCID from response> |  | 2g |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | CWS | TS\_CWS\_SOAP\_V1\_SIMPROVISIONING | MSISDN=($MSISDN) IMSI=($IMSI) SIMTYPE=($SIMTYPE\_($SUB\_BRAND)) PREPAIDINDICATOR=($CWS\_ACCOUNT\_TYPE) VERSION=WBA0703 TECHINDICATOR=LTE ICCID=($ISM\_ICCID) |  | Pre-Execution: IFNOTEXIST(EXEC\_CWS\_SIMPROVISIONING), SKIPTASK |  | 3g |  |
| RFS\_MPVOICE\_INTRA | ADD | OOCS | TS\_OCS\_HUAWEI\_V500R005C60LG0022\_createSubscriber | MSISDN1=($MSISDN) REGISTERCUSTOMER\_OPTYPE=1 REGISTERCUSTOMER\_CUSTKEY=($NP\_MSISDN) CUSTBASICINFO\_CUSTLEVEL=1 CREATESUBSCRIBERREQUEST\_ACCOUNT\_1=YES ACCOUNT\_ACCTKEY\_1=($NP\_MSISDN) ACCTINFO\_ACCTCODE\_1=($NP\_MSISDN) ACCTBASICINFO\_ACCTNAME\_1=($NP\_MSISDN) ACCTBASICINFO\_BILLLANG\_1=2011 ACCTBASICINFO\_DUNNINGFLAG\_1=1 ACCTBASICINFO\_FREEBILLMEDIUM\_1\_1=YES FREEBILLMEDIUM\_BMCODE\_1\_1=1 FREEBILLMEDIUM\_BMTYPE\_1\_1=1 ACCTINFO\_BILLCYCLETYPE\_1=01 ACCTINFO\_ACCTTYPE\_1=1 ACCTINFO\_PAYMENTTYPE\_1=0 ACCTINFO\_ACCTCLASS\_1=1 ACCTINFO\_CURRENCYID\_1=1117 ACCTINFO\_INITBALANCE\_1=0 ACCTINFO\_ACCTPAYMETHOD\_1=1 SUBSCRIBER\_SUBSCRIBERKEY=($NP\_MSISDN) SUBBASICINFO\_WRITTENLANG=2011 SUBBASICINFO\_IVRLANG=2011 SUBBASICINFO\_SUBLEVEL=1 SUBBASICINFO\_DUNNINGFLAG=1 SUBSCRIBERINFO\_USERCUSTOMERKEY=($NP\_MSISDN) SUBSCRIBERINFO\_SUBIDENTITY\_1=YES SUBIDENTITY\_SUBIDENTITYTYPE\_1=1 SUBIDENTITY\_SUBIDENTITY\_1=($NP\_MSISDN) SUBIDENTITY\_PRIMARYFLAG\_1=1 SUBSCRIBERINFO\_SUBCLASS=1 SUBSCRIBERINFO\_NETWORKTYPE=1 SUBSCRIBERINFO\_STATUS=2 SUBPAYMENTMODE\_PAYMENTMODE=0 SUBPAYMENTMODE\_PAYRELATIONKEY=($NP\_MSISDN) SUBPAYMENTMODE\_ACCTKEY=($NP\_MSISDN) OFFERINGKEY\_OFFERINGID1=($PRIMARY\_OFFER\_ID) PRIMARYOFFERING\_BUNDLEDFLAG=S PRIMARYOFFERING\_OFFERINGCLASS=I |  |  | <CreateSubscriberRequest>  <ns4:RegisterCustomer OpType="1">  <ns4:CustKey><NON63MSISDN></ns4:CustKey>  <ns4:CustInfo>  <ns3:CustBasicInfo>  <ns3:CustLevel>1</ns3:CustLevel>  </ns3:CustBasicInfo>  </ns4:CustInfo>  </ns4:RegisterCustomer>  <ns4:Account>  <ns4:AcctKey><NON63MSISDN></ns4:AcctKey>  <ns4:AcctInfo>  <ns3:AcctCode><NON63MSISDN></ns3:AcctCode>  <ns3:AcctBasicInfo>  <ns3:AcctName><NON63MSISDN></ns3:AcctName>  <ns3:BillLang>2011</ns3:BillLang>  <ns3:DunningFlag>1</ns3:DunningFlag>  <ns3:FreeBillMedium>  <ns3:BMCode>1</ns3:BMCode>  <ns3:BMType>1</ns3:BMType>  </ns3:FreeBillMedium>  </ns3:AcctBasicInfo>  <ns3:BillCycleType>01</ns3:BillCycleType>  <ns3:AcctType>1</ns3:AcctType>  <ns3:PaymentType>0</ns3:PaymentType>  <ns3:AcctClass>1</ns3:AcctClass>  <ns3:CurrencyID>1117</ns3:CurrencyID>  <ns3:InitBalance>0</ns3:InitBalance>  <ns3:AcctPayMethod>1</ns3:AcctPayMethod>  </ns4:AcctInfo>  </ns4:Account>  <ns4:Subscriber>  <ns4:SubscriberKey><NON63MSISDN></ns4:SubscriberKey>  <ns4:SubscriberInfo>  <ns3:SubBasicInfo>  <ns3:WrittenLang>2011</ns3:WrittenLang>  <ns3:IVRLang>2011</ns3:IVRLang>  <ns3:SubLevel>1</ns3:SubLevel>  <ns3:DunningFlag>1</ns3:DunningFlag>  </ns3:SubBasicInfo>  <ns3:UserCustomerKey><NON63MSISDN></ns3:UserCustomerKey>  <ns3:SubIdentity>  <ns3:SubIdentityType>1</ns3:SubIdentityType>  <ns3:SubIdentity><NON63MSISDN></ns3:SubIdentity>  <ns3:PrimaryFlag>1</ns3:PrimaryFlag>  </ns3:SubIdentity>  <ns3:SubClass>1</ns3:SubClass>  <ns3:NetworkType>1</ns3:NetworkType>  <ns3:Status>1</ns3:Status>  </ns4:SubscriberInfo>  <ns4:SubPaymentMode>  <ns4:PaymentMode>0</ns4:PaymentMode>  <ns4:PayRelationKey><NON63MSISDN></ns4:PayRelationKey>  <ns4:AcctKey><NON63MSISDN></ns4:AcctKey>  </ns4:SubPaymentMode>  </ns4:Subscriber>  <ns4:PrimaryOffering>  <ns3:OfferingKey>  <ns3:OfferingID><primary\_offer\_id></ns3:OfferingID>  </ns3:OfferingKey>  <ns3:BundledFlag>S</ns3:BundledFlag>  <ns3:OfferingClass>I</ns3:OfferingClass>  </ns4:PrimaryOffering> </CreateSubscriberRequest> | 1 | <SubDeactivationRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>3</ns8:OpType> </SubDeactivationRequest> |
| RFS\_MPVOICE\_INTRA | ADD | OOCS | TS\_OCS\_HUAWEI\_V500R005C60LG0022\_changeSubInfo | SUBACCESSCODE\_PRIMARYIDENTITY=($NP\_MSISDN) WELCOME\_PACK=($WELCOME\_PACK) |  |  | <ChangeSubInfoRequest>  <ns4:SubAccessCode>  <ns3:PrimaryIdentity><NON63MSISDN></ns3:PrimaryIdentity>  </ns4:SubAccessCode>  <ns4:SubBasicInfo>  <ns3:SubProperty>  <ns3:Code>C\_N\_WELCOMEPACKAGE</ns3:Code>  <ns3:Value><WELCOME\_PACK></ns3:Value>  </ns3:SubProperty>  </ns4:SubBasicInfo> </ChangeSubInfoRequest> | 2 |  |
| RFS\_MPVOICE\_INTRA | ADD | HLR | TS\_HLR\_ONENDS\_V9\_DUMMY | USE\_TEMPLATE=MPVOICE\_INTRA\_ADD\_($HLR\_CAMPUS)\_($SUB\_BRAND) IMSI1=($IMSI) MSISDN1=($MSISDN) |  |  | NOTE: This varies depending to CRI inquire if IDC or Cebu and sub\_brand PLTEL or PPAID  PLTEL IDC <spml:batchRequest  xmlns:spml="urn:siemens:names:prov:gw:SPML:2:0"  xmlns:subscriber="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" execution="synchronous" onError="exit\_rollback" processing="sequential" xsi:schemaLocation="urn:siemens:names:prov:gw:SUBSCRIBER:3:0 subscriber-3.0.xsd">  <version>SUBSCRIBER\_v30</version>  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <osb1>false</osb1>  <osb2>false</osb2>  <osb3>true</osb3>  <osb4>false</osb4>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <sr>9</sr>  <ts11>  <msisdn>${MSISDN1}</msisdn>  </ts11>  <ts21>  <msisdn>${MSISDN1}</msisdn>  </ts21>  <ts22>  <msisdn>${MSISDN1}</msisdn>  </ts22>  <bs20genr>  <msisdn>${MSISDN1}</msisdn>  </bs20genr>  <bs30genr>  <msisdn>${MSISDN1}</msisdn>  </bs30genr>  <gprs>  <msisdn>${MSISDN1}</msisdn>  </gprs>  <caw/>  <baoc/>  <boic/>  <boicexhc/>  <baic/>  <bicroam/>  <cuss>  <status>2</status>  </cuss>  <basicSelfLocation>  <status>2</status>  </basicSelfLocation>  <optimalRouting>true</optimalRouting>  <ndcLac>908</ndcLac>  <routingCategory>32</routingCategory>  <supportNewRadioSecondaryRAT>true</supportNewRadioSecondaryRAT>  </valueObject>  </modification>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <generalChargingCharacteristics>  <chargingCharacteristicsProfile>4</chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior>5</chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <odbgprs>0</odbgprs>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:COMCB">  <control>byOperator</control>  </valueObject>  </modification>  <modification name="hlr" operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbsci>2</odbsci>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>3</id>  <type>2</type>  <qosProfile>QOS11</qosProfile>  <apn>talkntext</apn>  <apnArea>HPLMN</apnArea>  <extType>5</extType>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>3</defaultPdnContextId>  <maxBandwidthUp>2000000000</maxBandwidthUp>  <maxBandwidthDown>2000000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn>${MSISDN1}</msisdn>  </eps>  <epsPdnContext>  <apn>talkntext</apn>  <contextId>3</contextId>  <type>both</type>  <maxBandwidthUp>2000000000</maxBandwidthUp>  <maxBandwidthDown>2000000000</maxBandwidthDown>  <qos>LteQos</qos>  </epsPdnContext>  </valueObject>  </modification>  </request>  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification name="eir" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EIR"/>  </modification>  </request> </spml:batchRequest>   PPAID IDC <spml:batchRequest  xmlns:spml="urn:siemens:names:prov:gw:SPML:2:0"  xmlns:subscriber="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" execution="synchronous" processing="sequential" onError="exit\_rollback" xsi:schemaLocation="urn:siemens:names:prov:gw:SUBSCRIBER:3:0 subscriber-3.0.xsd">  <version>SUBSCRIBER\_v30</version>  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <osb1>false</osb1>  <osb2>false</osb2>  <osb3>true</osb3>  <osb4>false</osb4>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <rr>RPI\_all</rr>  <sr>1</sr>  <ts11>  <msisdn>${MSISDN1}</msisdn>  </ts11>  <ts21>  <msisdn>${MSISDN1}</msisdn>  </ts21>  <ts22>  <msisdn>${MSISDN1}</msisdn>  </ts22>  <bs20genr>  <msisdn>${MSISDN1}</msisdn>  </bs20genr>  <bs30genr>  <msisdn>${MSISDN1}</msisdn>  </bs30genr>  <gprs>  <msisdn>${MSISDN1}</msisdn>  </gprs>  <caw></caw>  <baoc></baoc>  <boic></boic>  <boicexhc></boicexhc>  <baic></baic>  <bicroam></bicroam>  <cuss>  <status>2</status>  </cuss>  <basicSelfLocation>  <status>2</status>  </basicSelfLocation>  <optimalRouting>true</optimalRouting>  <ndcLac>908</ndcLac>  <routingCategory>62</routingCategory>  <supportNewRadioSecondaryRAT>true</supportNewRadioSecondaryRAT>  </valueObject>  </modification>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <generalChargingCharacteristics>  <chargingCharacteristicsProfile>4</chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior>1</chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:COMCB">  <control>byOperator</control>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>2</id>  <type>2</type>  <qosProfile>QOS1</qosProfile>  <apn>INTERNET</apn>  <apnArea>HPLMN</apnArea>  <extType>5</extType>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>1</id>  <type>2</type>  <qosProfile>QOS1</qosProfile>  <apn>SMARTLTE</apn>  <apnArea>HPLMN</apnArea>  <extType>5</extType>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1845</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification name="hlr/roamSubscription" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:ROAMSUBSCRIPTION">  <roamSubscriptionInfo>RSI\_SPP10</roamSubscriptionInfo>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>1</defaultPdnContextId>  <maxBandwidthUp>2000000000</maxBandwidthUp>  <maxBandwidthDown>2000000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn>${MSISDN1}</msisdn>  </eps>  <epsPdnContext>  <apn>INTERNET</apn>  <contextId>2</contextId>  <type>both</type>  <maxBandwidthUp>2000000000</maxBandwidthUp>  <maxBandwidthDown>2000000000</maxBandwidthDown>  <qos>LteQos</qos>  </epsPdnContext>  <epsPdnContext>  <apn>SMARTLTE</apn>  <contextId>1</contextId>  <type>both</type>  <maxBandwidthUp>2000000000</maxBandwidthUp>  <maxBandwidthDown>2000000000</maxBandwidthDown>  <qos>LteQos</qos>  </epsPdnContext>  </valueObject>  </modification>  </request>  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification name="eir" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EIR"/>  </modification>  </request> </spml:batchRequest>   PLTEL Cebu <spml:batchRequest  xmlns:spml="urn:siemens:names:prov:gw:SPML:2:0"  xmlns:subscriber="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" execution="synchronous" onError="exit\_rollback" processing="sequential" xsi:schemaLocation="urn:siemens:names:prov:gw:SUBSCRIBER:3:0 subscriber-3.0.xsd">  <version>SUBSCRIBER\_v30</version>  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <osb1>false</osb1>  <osb2>false</osb2>  <osb3>true</osb3>  <osb4>false</osb4>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <sr>9</sr>  <ts11>  <msisdn>${MSISDN1}</msisdn>  </ts11>  <ts21>  <msisdn>${MSISDN1}</msisdn>  </ts21>  <ts22>  <msisdn>${MSISDN1}</msisdn>  </ts22>  <bs20genr>  <msisdn>${MSISDN1}</msisdn>  </bs20genr>  <bs30genr>  <msisdn>${MSISDN1}</msisdn>  </bs30genr>  <gprs>  <msisdn>${MSISDN1}</msisdn>  </gprs>  <caw/>  <baoc/>  <boic/>  <boicexhc/>  <baic/>  <bicroam/>  <cuss>  <status>2</status>  </cuss>  <basicSelfLocation>  <status>2</status>  </basicSelfLocation>  <optimalRouting>true</optimalRouting>  <ndcLac>908</ndcLac>  <routingCategory>32</routingCategory>  <supportNewRadioSecondaryRAT>true</supportNewRadioSecondaryRAT>  </valueObject>  </modification>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <generalChargingCharacteristics>  <chargingCharacteristicsProfile>4</chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior>5</chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <odbgprs>0</odbgprs>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:COMCB">  <control>byOperator</control>  </valueObject>  </modification>  <modification name="hlr" operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbsci>2</odbsci>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>3</id>  <type>2</type>  <qosProfile>QOS11</qosProfile>  <apn>talkntext</apn>  <apnArea>HPLMN</apnArea>  <extType>5</extType>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>3</defaultPdnContextId>  <maxBandwidthUp>2000000000</maxBandwidthUp>  <maxBandwidthDown>2000000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn>${MSISDN1}</msisdn>  </eps>  <epsPdnContext>  <apn>talkntext</apn>  <contextId>3</contextId>  <type>both</type>  <maxBandwidthUp>2000000000</maxBandwidthUp>  <maxBandwidthDown>2000000000</maxBandwidthDown>  <qos>LteQos</qos>  </epsPdnContext>  </valueObject>  </modification>  </request>  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification name="eir" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EIR"/>  </modification>  </request> </spml:batchRequest>   PPAID Cebu <spml:batchRequest  xmlns:spml="urn:siemens:names:prov:gw:SPML:2:0"  xmlns:subscriber="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" execution="synchronous" processing="sequential" onError="exit\_rollback" xsi:schemaLocation="urn:siemens:names:prov:gw:SUBSCRIBER:3:0 subscriber-3.0.xsd">  <version>SUBSCRIBER\_v30</version>  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <ntype>single</ntype>  <mobileSubscriberType>genericSubscriber</mobileSubscriberType>  <umtsSubscriber>  <accTypeGSM>true</accTypeGSM>  <accTypeGERAN>true</accTypeGERAN>  <accTypeUTRAN>true</accTypeUTRAN>  </umtsSubscriber>  <wllSubscriber>false</wllSubscriber>  <mscat>10</mscat>  <osb1>false</osb1>  <osb2>false</osb2>  <osb3>true</osb3>  <osb4>false</osb4>  <clip>true</clip>  <clipOverride>false</clipOverride>  <colpOverride>false</colpOverride>  <hold>true</hold>  <rr>RPI\_all</rr>  <sr>1</sr>  <ts11>  <msisdn>${MSISDN1}</msisdn>  </ts11>  <ts21>  <msisdn>${MSISDN1}</msisdn>  </ts21>  <ts22>  <msisdn>${MSISDN1}</msisdn>  </ts22>  <bs20genr>  <msisdn>${MSISDN1}</msisdn>  </bs20genr>  <bs30genr>  <msisdn>${MSISDN1}</msisdn>  </bs30genr>  <gprs>  <msisdn>${MSISDN1}</msisdn>  </gprs>  <caw></caw>  <baoc></baoc>  <boic></boic>  <boicexhc></boicexhc>  <baic></baic>  <bicroam></bicroam>  <cuss>  <status>2</status>  </cuss>  <basicSelfLocation>  <status>2</status>  </basicSelfLocation>  <optimalRouting>true</optimalRouting>  <ndcLac>908</ndcLac>  <routingCategory>62</routingCategory>  <supportNewRadioSecondaryRAT>true</supportNewRadioSecondaryRAT>  </valueObject>  </modification>  <modification operation="addorset">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:HLR">  <generalChargingCharacteristics>  <chargingCharacteristicsProfile>4</chargingCharacteristicsProfile>  <chargingCharacteristicsBehavior>1</chargingCharacteristicsBehavior>  </generalChargingCharacteristics>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:COMCB">  <control>byOperator</control>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>2</id>  <type>2</type>  <qosProfile>QOS1</qosProfile>  <apn>INTERNET</apn>  <apnArea>HPLMN</apnArea>  <extType>5</extType>  </valueObject>  </modification>  <modification operation="add" scope="uniqueTypeMapping">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:PDPContext">  <id>1</id>  <type>2</type>  <qosProfile>QOS1</qosProfile>  <apn>SMARTLTE</apn>  <apnArea>HPLMN</apnArea>  <extType>5</extType>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:OCSI">  <operatorServiceName>O-CSI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification operation="add">  <valueObject  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="subscriber:SMSCSI">  <operatorServiceName>SMSCI1849</operatorServiceName>  <csiState>1</csiState>  <csiNotify>2</csiNotify>  </valueObject>  </modification>  <modification name="hlr/roamSubscription" operation="addorset"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:ROAMSUBSCRIPTION">  <roamSubscriptionInfo>RSI\_SPP10</roamSubscriptionInfo>  </valueObject>  </modification>  <modification operation="setoradd">  <valueObject xsi:type="subscriber:HLR">  <eps>  <defaultPdnContextId>1</defaultPdnContextId>  <maxBandwidthUp>2000000000</maxBandwidthUp>  <maxBandwidthDown>2000000000</maxBandwidthDown>  <apnOIReplacement>mnc003.mcc515.gprs</apnOIReplacement>  <sessionTimeout>3600</sessionTimeout>  <accessAPNEnabled>true</accessAPNEnabled>  <mipFeatureVector>assign\_local\_ip</mipFeatureVector>  <mipFeatureVector>mip6\_integrated</mipFeatureVector>  <msisdn>${MSISDN1}</msisdn>  </eps>  <epsPdnContext>  <apn>INTERNET</apn>  <contextId>2</contextId>  <type>both</type>  <maxBandwidthUp>2000000000</maxBandwidthUp>  <maxBandwidthDown>2000000000</maxBandwidthDown>  <qos>LteQos</qos>  </epsPdnContext>  <epsPdnContext>  <apn>SMARTLTE</apn>  <contextId>1</contextId>  <type>both</type>  <maxBandwidthUp>2000000000</maxBandwidthUp>  <maxBandwidthDown>2000000000</maxBandwidthDown>  <qos>LteQos</qos>  </epsPdnContext>  </valueObject>  </modification>  </request>  <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier>${IMSI1}</identifier>  <modification name="eir" operation="addorset" scope="uniqueTypeMapping"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">  <valueObject xsi:type="subscriber:EIR"/>  </modification>  </request> </spml:batchRequest> | 2 | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/> </request> |
| RFS\_MPVOICE\_INTRA | ADD\_NC | MPCC | TS\_MPCC\_FILE\_V1\_CreateMpcc | MSISDN=($MSISDN) BRAND=($BRAND) TYPE=($ACCOUNT\_TYPE) |  |  | <MSISDN>|<BRAND>|<TYPE>|<REFERENCE ID> | 1a |  |
| RFS\_MPVOICE\_INTRA | ADD\_NC | ISM | TS\_ISM\_SOAP\_V1\_changeBrand | MSISDN1=($MSISDN) BRAND\_CODE=($SUB\_BRAND) |  |  | <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:web="http://web.external.ism.eai.mt.com/">  <soapenv:Header/>  <soapenv:Body>  <web:changeBrand>  <web:changeBrandRequest>  <headerData>  <username>wsuser</username>  <password>abcdefg123456</password>  <transactionId></transactionId>  </headerData>  <iccid></iccid>  <imsi></imsi>  <msisdn>MSISDN</msisdn>  <brandCode>Brand (need to tranlate to ISM Brand) </brandCode>  <subBrand>subrand (need to translate to ISM Brand) </subBrand>  <remarks></remarks>  </web:changeBrandRequest>  </web:changeBrand>  </soapenv:Body> </soapenv:Envelope> | 1b |  |
| RFS\_MPVOICE\_INTRA | ADD\_NC | ISM | TS\_ISM\_SOAP\_V1\_changeBillingCycle | MSISDN1=($MSISDN) BILLING\_TYPE=($ISM\_BILLING\_TYPE) |  | Pre-Execution: MAP(ISM\_BILLING\_TYPE=($ACCOUNT\_TYPE)),STR\_UPPER(ISM\_BILLING\_TYPE) | <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:web="http://web.external.ism.eai.mt.com/">  <soapenv:Header/>  <soapenv:Body>  <web:changeBillingType>  <web:changeBillingTypeRequest>  <headerData>  <username>wsuser</username>  <password> abcdefg123456</password>  <transactionId>1234</transactionId>  </headerData>  <iccid></iccid>  <imsi></imsi>  <msisdn>MSISDN</msisdn>  <billingType>account\_type</billingType>  <remarks></remarks>  </web:changeBillingTypeRequest>  </web:changeBillingType>  </soapenv:Body> </soapenv:Envelope> | 1c |  |
| RFS\_MPVOICE\_INTRA | ADD\_NC | CDP | TS\_CDP\_XML\_V1\_SYNCUSERDATA | PAY\_TYPE=($CDP\_PAY\_TYPE) USER\_BRAND=($ROUTCAT) USERID\_TYPE=0 |  | Pre-Execution: IF $ACCOUNT\_TYPE==Postpaid MAP CDP\_PAY\_TYPE=0 ELSEIF $ACCOUNT\_TYPE==Prepaid MAP CDP\_PAY\_TYPE=1 | POST /bme/services/SISService HTTP/1.1 Content-Length: 5438 Content-Type: text/xml;charset=utf-8 SOAPAction: "" User-Agent: Java/1.6.0\_10-rc2 Host: 10.137.213.127:21322 Accept: text/html, image/gif, image/jpeg, \*; q=.2, \*/\*; q=.2 Connection: keep-alive  <?xml version="1.0" encoding="utf-8"?> <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:xsd="http://www.w3.org/2001/XMLSchema" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"> <soapenv:Header>  <ns1:IBSoapHeader soapenv:actor="http://schemas.xmlsoap.org/soap/actor/next" soapenv:mustUnderstand="0" xmlns:ns1="http://soapheader.ib.sdp.huawei.com">  <ns1:version>V1.0</ns1:version>  <ns1:traceUniqueID>000000102651206180843180001001</ns1:traceUniqueID>  <ns1:sourceDeviceType>23</ns1:sourceDeviceType>  <ns1:sourceDeviceCode>2300000001</ns1:sourceDeviceCode>  <ns1:destDeviceType>0</ns1:destDeviceType>  <ns1:destDeviceCode>0000000001</ns1:destDeviceCode> <ns1:authenticatorSource>9d32d1185baa0883d9fd9c86ffeed7e92c38fd4770265f2a8e09466294a0c502</ns1:authenticatorSource>  <ns1:timeStamp>20191014162246</ns1:timeStamp>  </ns1:IBSoapHeader> </soapenv:Header>  <soapenv:Body>  <in0 xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <extensionInfo xmlns="http://struct.soap.ccengine.mdsp.huawei.com">  <namedParameters xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <item xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <key xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">who am I?</key>  <value xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">WWWW</value>  </item>  </namedParameters>  </extensionInfo>  <version xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">V1.0</version>  <transactionID xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">OrderNO</transactionID>  <updateType xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">Modify</updateType>  <userID xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <ID>MSISDN</ID>  <type>0</type>  </userID>  <userProfile xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <extensionInfo xmlns="http://struct.soap.ccengine.mdsp.huawei.com">  <namedParameters xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <item xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <key xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">isRoam</key>  <value xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">1</value>  </item>  </namedParameters>  </extensionInfo>  <userName>fine</userName>  <payType>account\_type ( 0 Postpaid 1 prepaid) </payType> <userBrand> routecat from Optima </userBrand>  <userID>  <ID>MSISDN</ID>  <type>0</type>  </userID>  <userState>0</userState>  <userType>0</userType>  <userSID>12345</userSID>  </userProfile>  </in0>  </soapenv:Body> </soapenv:Envelope> | 1d |  |
| RFS\_MPVOICE\_INTRA | ADD\_NC | AGW | TS\_AGW\_SOAP\_V1\_SYNCUSERDATA | PAY\_TYPE=($AGW\_PAY\_TYPE) USER\_BRAND=($ROUTCAT) |  | Pre-Execution: IF $ACCOUNT\_TYPE==Postpaid MAP AGW\_PAY\_TYPE=0 ELSEIF $ACCOUNT\_TYPE==Prepaid MAP AGW\_PAY\_TYPE=1 | POST /bme/services/SISService HTTP/1.1 Content-Length: 5438 Content-Type: text/xml;charset=utf-8 SOAPAction: "" User-Agent: Java/1.6.0\_10-rc2 Host: 10.137.213.127:21322 Accept: text/html, image/gif, image/jpeg, \*; q=.2, \*/\*; q=.2 Connection: keep-alive  <?xml version="1.0" encoding="utf-8"?> <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:xsd="http://www.w3.org/2001/XMLSchema" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"> <soapenv:Header>  <ns1:IBSoapHeader soapenv:actor="http://schemas.xmlsoap.org/soap/actor/next" soapenv:mustUnderstand="0" xmlns:ns1="http://soapheader.ib.sdp.huawei.com">  <ns1:version>V1.0</ns1:version>  <ns1:traceUniqueID>000000102651206180843180001001</ns1:traceUniqueID>  <ns1:sourceDeviceType>23</ns1:sourceDeviceType>  <ns1:sourceDeviceCode>2300000001</ns1:sourceDeviceCode>  <ns1:destDeviceType>0</ns1:destDeviceType>  <ns1:destDeviceCode>0000000001</ns1:destDeviceCode> <ns1:authenticatorSource>9d32d1185baa0883d9fd9c86ffeed7e92c38fd4770265f2a8e09466294a0c502</ns1:authenticatorSource>  <ns1:timeStamp>20191014162246</ns1:timeStamp>  </ns1:IBSoapHeader> </soapenv:Header>  <soapenv:Body>  <in0 xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <extensionInfo xmlns="http://struct.soap.ccengine.mdsp.huawei.com">  <namedParameters xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <item xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <key xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">who am I?</key>  <value xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">WWWW</value>  </item>  </namedParameters>  </extensionInfo>  <version xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">V1.0</version>  <transactionID xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">OrderNO</transactionID>  <updateType xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">Modify</updateType>  <userID xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <ID>MSISDN</ID>  <type>0</type>  </userID>  <userProfile xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <extensionInfo xmlns="http://struct.soap.ccengine.mdsp.huawei.com">  <namedParameters xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">  <item xmlns="http://service.soap.ccengine.mdsp.huawei.com">  <key xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">isRoam</key>  <value xmlns="http://struct.soap.ccengine.mdsp.huawei.com/xsd">1</value>  </item>  </namedParameters>  </extensionInfo>  <userName>fine</userName>  <payType>account\_type ( 0 Postpaid 1 prepaid) </payType>  <userID>  <ID>MSISDN</ID>  <type>7</type>  </userID>  <userState>0</userState>  <userType>0</userType>  <userSID>12345</userSID>  </userProfile>  </in0>  </soapenv:Body> </soapenv:Envelope> | 1e |  |
| RFS\_MPVOICE\_INTRA | ADD\_NC | OTA | TS\_OTA\_OPENAPI\_V1\_get | HTTP\_REQUEST\_MSISDN=($MSISDN) | HTTP\_REQUEST\_ACCESS\_CODE=($BST\_ACCESS\_CODE) HTTP\_REQUEST\_KWD=($BST\_KEYWORD) HTTP\_REQUEST\_SVCID=($BST\_SERVICE\_ID) | Post-Execution: If error\_code == 0005 || 9999 SET MNP\_OTA\_ERROR\_FILE = TRUE |  | 1f |  |
| RFS\_MVOICE\_INTRA | ADD\_NC | OTA\_FILE | TS\_FILE\_FORMATPARSER\_ANY\_ota\_file | REQ\_TYPE=1 OPER\_TYPE=MNP\_OTA ACTION=MNP\_OTA MSISDN=($MSISDN) |  | Pre-Execution: If MNP\_OTA\_ERROR\_FILE ParamExist && MNP\_OTA\_ERROR\_FILE == TRUE, executeTask Else skiptask |  |  |  |
| RFS\_MPVOICE\_INTRA | ADD\_NC | CWS | TS\_CWS\_SOAP\_V1\_SIMCHANGEBRAND | MSISDN=($MSISDN) NEWSIMTYPE=($SIMTYPE\_($SUB\_BRAND)) NEWPREPAIDINDICATOR=($CWS\_ACCOUNT\_TYPE) |  | Pre-Execution: IF ($ACCOUNT\_TYPE)=='Postpaid' MAP CWS\_ACCOUNT\_TYPE='POST\_PAID' IF ($ACCOUNT\_TYPE)=='Prepaid' MAP CWS\_ACCOUNT\_TYPE='PREPAID' Post-Execution IF ($ERROR\_CODE)=='D067001' IGNOREFAIL, MAP EXEC\_SIMPROVISIONING=TRUE | <soapenv:Envelope xmlns:soapenv="http://schemas.xmlsoap.org/soap/envelope/" xmlns:sim="http://smart.com.ph/SimProv">  <soapenv:Header/>  <soapenv:Body>  <sim:SIMChangeBrandRequest>  <msisdn><MSISDN></msisdn>  <oldSimType><OLDSIMTYPE></oldSimType>  <newSimType><NEWSIMTYPE></newSimType>  <oldPrepaidIndicator><OLDPREPAIDINDICATOR></oldPrepaidIndicator>  <newPrepaidIndicator><NEWPREPAIDINDICATOR></newPrepaidIndicator>  </sim:SIMChangeBrandRequest>  </soapenv:Body> </soapenv:Envelope> | 1g |  |
| RFS\_MPVOICE\_INTRA | ADD\_NC | ISM | TS\_ISM\_SOAP\_V1\_getSimInfo | IMSI=($IMSI) |  | Pre-Execution: IF EXEC\_SIMPROVISIONING!=TRUE, SKIPTASK Post-Execution: ISM\_ICCID=<ICCID from response> |  | 2g |  |
| RFS\_MPVOICE\_INTRA | ADD\_NC | CWS | TS\_CWS\_SOAP\_V1\_SIMPROVISIONING | MSISDN=($MSISDN) IMSI=($IMSI) SIMTYPE=($SIMTYPE\_($SUB\_BRAND)) PREPAIDINDICATOR=($CWS\_ACCOUNT\_TYPE) VERSION=WBA0703 TECHINDICATOR=LTE ICCID=($ISM\_ICCID) |  | Pre-Execution: IF EXEC\_SIMPROVISIONING!=TRUE, SKIPTASK |  | 3g |  |
| RFS\_MVOICE\_INTRA | REMOVE | HLR | TS\_HLR\_ONENDS\_V9\_DUMMY | USE\_TEMPLATE=MVOICE\_INTRA\_REMOVE |  |  | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/> </request> |  |  |
| RFS\_MVOICE\_INTRA | REMOVE\_NC | SWiM (APTILO) | TS\_APTILO\_HTTP\_V2\_statusChange |  |  |  | {"msisdn":"<MSISDN>"} | 1a |  |
| RFS\_MPVOICE\_INTRA | REMOVE | OOCS | TS\_OCS\_HUAWEI\_V500R005C60LG0022\_changeSubOffering |  |  | 1. Should be able to support multiple values of OCS OFFER ID (pipe-delimited) 2. Execute separate transaction for each OCS OFFER ID | <ChangeSubOfferingRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:SupplementaryOffering>  <ns8:DelOffering>  <ns8:OfferingKey>  <ns7:OfferingID><primary\_offer\_id></ns7:OfferingID>  </ns8:OfferingKey>  </ns8:DelOffering>  </ns8:SupplementaryOffering>  <ns8:HandlingChargeFlag>1</ns8:HandlingChargeFlag> </ChangeSubOfferingRequest> |  | <ChangeSubOfferingRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:SupplementaryOffering>  <ns8:AddOffering>  <ns7:OfferingKey>  <ns7:OfferingID><OCS OFFER ID></ns7:OfferingID>  </ns7:OfferingKey>  <ns8:EffectiveTime>  <ns7:Mode>I</ns7:Mode>  </ns8:EffectiveTime>  <ns8:ActivationTime/>  </ns8:AddOffering>  </ns8:SupplementaryOffering> </ChangeSubOfferingRequest> |
| RFS\_MPVOICE\_INTRA | REMOVE | OOCS | TS\_OCS\_HUAWEI\_V500R005C60LG0022\_subDeactivation |  |  | 1. Whitelist error code 118030349. | <SubDeactivationRequest>  <ns8:SubAccessCode>  <ns7:PrimaryIdentity><NON63MSISDN></ns7:PrimaryIdentity>  </ns8:SubAccessCode>  <ns8:OpType>3</ns8:OpType> </SubDeactivationRequest> |  |  |
| RFS\_MPVOICE\_INTRA | REMOVE | HLR | TS\_HLR\_ONENDS\_V9\_DUMMY | USE\_TEMPLATE=MPVOICE\_INTRA\_REMOVE |  |  | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr" operation="remove"/> </request> |  |  |
| RFS\_MPVOICE\_INTRA | REMOVE\_NC | ISM | TS\_ISM\_Inquire\_getMsisdnInfo | ACTION=GET\_MSISDN\_INFO IMSI=($IMSI) |  | Post-Execution: ISM\_ICCID=<ICCID from response> ISM\_HLR=<HLR\_CODE from response> |  | 1a |  |
| RFS\_MPVOICE\_INTRA | REMOVE\_NC | EDB | TS\_FILE\_FORMATPARSER\_ANY\_edb | CONTENT\_TYPE = ($MSISDN) ACTION=EDB\_FILE OPER\_TYPE=EDB MSISDN=($MSISDN) IMSI=($IMSI) HLR=($ISM\_HLR) IDX\_CODE=($ISM\_IDX\_CODE) ICCID=($ISM\_ICCID) FILE\_DATE=($MNP\_TIMESTAMP) | FILE\_DATE = sysdate(YYYYMMDDHHMISSss) | get the HLR and ICCID from ISM\_Inquire Post-Execution: EDB\_FILENAME=($@NEW@FILENAME) EDB\_LOCAL\_DIR=($@NEW@LOCAL\_DIR) | File Content Format: space delimited <MIN 63-format> <IMSI> HLR<HLR#(query ISM to retrieve HLR)> <IDX\_CODE(Sub brand)> <ICCID(query ISM to retrieve ICCID)>  Example: 639462193415 515031417343407 HLRG14 PLTEL 89630314062143884186 | 1b |  |
| RFS\_MPVOICE\_INTRA | REMOVE\_NC | EDB | TS\_FILE\_FORMATPARSER\_ANY\_edb | CONTENT\_TYPE = ($MSISDN) ACTION=EDB\_FILE\_CONCAT OPER\_TYPE=EDB MSISDN=($MSISDN) IMSI=($IMSI) HLR=($ISM\_HLR) IDX\_CODE=($ISM\_IDX\_CODE) ICCID=($ISM\_ICCID) FILE\_DATE=($MNP\_TIMESTAMP) | FILE\_DATE = sysdate(YYYYMMDDHHMISSss) | get the HLR and ICCID from ISM\_Inquire Post-Execution: EDB\_FILENAME=($@NEW@FILENAME) EDB\_LOCAL\_DIR=($@NEW@LOCAL\_DIR) | File Content Format: space delimited <MIN 63-format> <IMSI> HLR<HLR#(query ISM to retrieve HLR)> <IDX\_CODE(Sub brand)> <ICCID(query ISM to retrieve ICCID)>  Example: 639462193415 515031417343407 HLRG14 PLTEL 89630314062143884186 | 1c |  |
| RFS\_MPVOICE\_INTRA | REMOVE\_NC | EDB | TS\_FTP\_FILE\_ANY\_transferFileToRemote\_sftp\_edb | BACKUP\_DIR=($EDB\_LOCAL\_DIR) FILE\_AMOUNT=1 FILENAME=($EDB\_FILENAME) LOCAL\_DIR=($EDB\_LOCAL\_DIR) NE\_ID=($FTP\_EDB\_NE\_ID) REMOTE\_DIR=($EDB\_REMOTE\_DIR) TRANSFER\_MODE=1 |  |  |  | 1d |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Catalog item** | **Transaction** | **NETWORK ELEMENT** | **Parameters/Attributes Internal to USPS** | **ACTIONCODE/CONDITION** |
| RFS\_MVOICE | ADD | DP9 | is\_home\_wifi | 1. If is\_home\_wifi is set to 'Y', no need to execute DP9, CWS and FMS commands. 2. If is\_home\_wifi is set to 'N', or is not included in the request, treat request as regular wireless and target HLR, DP9, OneOCS, SSP, CWS, ISM, FMS. |
| RFS\_MVOICE | ADD | CWS | is\_home\_wifi |  |
| RFS\_MVOICE | ADD | FMS | is\_home\_wifi |  |
| RFS\_MVOICE | CHGIMSI | ONEOCS | is\_home\_wifi | 1. If is\_home\_wifi is set to 'Y', no need to execute OneOCS, CWS and FMS. 2. If is\_home\_wifi is set to 'N', or is not included in the request, treat request as regular wireless and target HLR, OneOCS, SSP, CWS, ISM, FMS. |
| RFS\_MVOICE | CHGIMSI | CWS | is\_home\_wifi |  |
| RFS\_MVOICE | CHGIMSI | FMS | is\_home\_wifi |  |
| RFS\_MVOICE | REMOVE | DP9 | is\_home\_wifi | If is\_home\_wifi is set to 'Y', don't execute DP9 command. |
| RFS\_MVOICE | REMOVE | APTILO | is\_home\_wifi | If is\_home\_wifi is set to 'Y', don't execute APTILO command. |
| RFS\_MVOICE | REMOVE | CDP | is\_home\_wifi | If is\_home\_wifi is set to 'Y', don't execute CDP command. |
| RFS\_MVOICE | REMOVE | MYSMRT | is\_home\_wifi | If is\_home\_wifi is set to 'Y', don't execute MYSMRT command. |
| RFS\_MVOICE | REMOVE | FMS | is\_home\_wifi | If is\_home\_wifi is set to 'Y', don't execute FMS command. |
| RFS\_DATA | SUSPEND | HLR | is\_home\_wifi | If is\_home\_wifi is set to 'Y', no need to execute HLR |
| RFS\_DATA | RESUME | HLR | is\_home\_wifi | If is\_home\_wifi is set to 'Y', no need to execute HLR |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **<RFS>\_<ACTION>** | **SPML** | **Parameters** | **Rollback** |  |
| DATA\_ADD | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>1</odbgprs>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:PDPContext">  <id><PDP ID></id>  <type>2</type>  <qosProfile><QOS></qosProfile>  <apn><APN NAME></apn>  <apnArea>HPLMN</apnArea>  <extType>5</extType>  </valueObject>  </modification> </request> | IMSI PDP ID, QOS, APN NAME | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>2</odbgprs>  </valueObject>  </modification>  <modification name="hlr/pdpContext[@apn='<APN NAME>']" operation="remove"></modification> </request> |  |
| DATA\_REMOVE | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>2</odbgprs>  </valueObject>  </modification>  <modification name="hlr/pdpContext[@apn='<APN NAME>']" operation="remove"></modification> </request> | IMSI PDP ID, QOS, APN NAME | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>1</odbgprs>  </valueObject>  </modification>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:PDPContext">  <id><PDP ID></id>  <type>2</type>  <qosProfile><QOS></qosProfile>  <apn><APN NAME></apn>  <apnArea>HPLMN</apnArea>  <extType>5</extType>  </valueObject>  </modification> </request> |  |
| DATA\_RESUME | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>1</odbgprs>  </valueObject>  </modification> </request> | IMSI | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>2</odbgprs>  </valueObject>  </modification> </request> |  |
| DATA\_SUSPEND | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>2</odbgprs>  </valueObject>  </modification> </request> | IMSI | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>1</odbgprs>  </valueObject>  </modification> </request> |  |
| LTE\_RESUME | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps>VPLMNAP</odbPOAccessEps>  </valueObject>  </modification> </request> | IMSI | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps>ALLPOS</odbPOAccessEps>  </valueObject>  </modification> </request> |  |
| LTE\_SUSPEND | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps>ALLPOS</odbPOAccessEps>  </valueObject>  </modification> </request> | IMSI | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps>VPLMNAP</odbPOAccessEps>  </valueObject>  </modification> </request> |  |
| DATAROAMING\_RESUME | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>0</odbgprs>  </valueObject>  </modification>  <modification name="hlr/eps/odbPOAccessEps" operation="remove" scope="uniqueTypeMapping"/> </request> | IMSI | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>2</odbgprs>  </valueObject>  </modification>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps>ALLPOS</odbPOAccessEps>  </valueObject>  </modification> </request> | Note: Create new catalog txn and HLR template |
| DATAROAMING\_SUSPEND | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>2</odbgprs>  </valueObject>  </modification>  <modification name="hlr/eps" operation="addorset" scope="uniqueTypeMapping">  <valueObject  xmlns:ns2="urn:siemens:names:prov:gw:SUBSCRIBER:3:0"  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:type="ns2:EPS">  <odbPOAccessEps>ALLPOS</odbPOAccessEps>  </valueObject>  </modification> </request> | IMSI | <request xsi:type="spml:ModifyRequest">  <version>SUBSCRIBER\_v30</version>  <objectclass>Subscriber</objectclass>  <identifier><IMSI></identifier>  <modification operation="addorset" scope="uniqueTypeMapping">  <valueObject xsi:type="subscriber:HLR">  <odbgprs>0</odbgprs>  </valueObject>  </modification>  <modification name="hlr/eps/odbPOAccessEps" operation="remove" scope="uniqueTypeMapping"/> </request> |  |